,Mounting##Other##,Output##Other##,"CRI, CCT##Other##",Beam Spread##OTHER##,Housing Type##OTHER##,Model##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##Other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Voltage Comment##OTHER##,Photometric Web File##OTHER##,Instruction Sheet Link##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,C Housing##OTHER##,C High Output##Other##,C Low Output##Other##,C Flanged##OTHER##
E2RL-LH82720AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2RL-LH82720AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH82720AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2RL-LH82720AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH82730AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2RL-LH82730AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH82730AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2RL-LH82730AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH82740AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2RL-LH82740AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH82740AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2RL-LH82740AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH82760AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2RL-LH82760AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH82760AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2RL-LH82760AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83020AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2RL-LH83020AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83020AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2RL-LH83020AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83030AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2RL-LH83030AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83030AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2RL-LH83030AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83040AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2RL-LH83040AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83040AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2RL-LH83040AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83060AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2RL-LH83060AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83060AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2RL-LH83060AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83520AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2RL-LH83520AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83520AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2RL-LH83520AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83530AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2RL-LH83530AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83530AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2RL-LH83530AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83540AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2RL-LH83540AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83540AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2RL-LH83540AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83560AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2RL-LH83560AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH83560AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2RL-LH83560AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,0
E2RL-LH92720AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2RL-LH92720AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH92720AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2RL-LH92720AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH92730AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2RL-LH92730AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH92730AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2RL-LH92730AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH92740AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2RL-LH92740AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH92740AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2RL-LH92740AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH92760AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2RL-LH92760AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH92760AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2RL-LH92760AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93020AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2RL-LH93020AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93020AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2RL-LH93020AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93030AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2RL-LH93030AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93030AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2RL-LH93030AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93040AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2RL-LH93040AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93040AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2RL-LH93040AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93060AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2RL-LH93060AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93060AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2RL-LH93060AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93520AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2RL-LH93520AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93520AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2RL-LH93520AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93530AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2RL-LH93530AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93530AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2RL-LH93530AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93540AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2RL-LH93540AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93540AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2RL-LH93540AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93560AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2RL-LH93560AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LH93560AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2RL-LH93560AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,0
E2RL-LO82720AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2RL-LO82720AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO82720AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2RL-LO82720AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO82730AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2RL-LO82730AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO82730AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2RL-LO82730AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO82740AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2RL-LO82740AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO82740AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2RL-LO82740AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO82760AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2RL-LO82760AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO82760AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2RL-LO82760AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83020AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2RL-LO83020AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83020AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2RL-LO83020AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83030AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2RL-LO83030AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83030AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2RL-LO83030AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83040AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2RL-LO83040AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83040AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2RL-LO83040AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83060AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2RL-LO83060AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83060AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2RL-LO83060AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83520AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2RL-LO83520AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83520AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2RL-LO83520AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83530AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2RL-LO83530AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83530AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2RL-LO83530AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83540AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2RL-LO83540AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83540AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2RL-LO83540AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83560AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2RL-LO83560AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO83560AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2RL-LO83560AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,0
E2RL-LO92720AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2RL-LO92720AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO92720AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2RL-LO92720AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO92730AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2RL-LO92730AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO92730AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2RL-LO92730AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO92740AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2RL-LO92740AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO92740AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2RL-LO92740AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO92760AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2RL-LO92760AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO92760AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2RL-LO92760AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93020AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2RL-LO93020AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93020AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2RL-LO93020AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93030AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2RL-LO93030AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93030AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2RL-LO93030AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93040AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2RL-LO93040AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93040AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2RL-LO93040AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93060AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2RL-LO93060AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93060AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2RL-LO93060AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93520AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2RL-LO93520AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93520AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2RL-LO93520AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93530AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2RL-LO93530AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93530AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2RL-LO93530AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93540AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2RL-LO93540AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93540AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2RL-LO93540AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93560AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2RL-LO93560AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO93560AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2RL-LO93560AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,0
E2RL-LO9WD20AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2RL-LO9WD20AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RL-LO9WD20AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2RL-LO9WD20AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RL-LO9WD30AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2RL-LO9WD30AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RL-LO9WD30AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2RL-LO9WD30AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RL-LO9WD40AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2RL-LO9WD40AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RL-LO9WD40AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2RL-LO9WD40AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RL-LO9WD60AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2RL-LO9WD60AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RL-LO9WD60AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2RL-LO9WD60AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,0
E2RF-LH82720AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2RF-LH82720AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH82720AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2RF-LH82720AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH82730AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2RF-LH82730AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH82730AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2RF-LH82730AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH82740AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2RF-LH82740AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH82740AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2RF-LH82740AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH82760AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2RF-LH82760AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH82760AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2RF-LH82760AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83020AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2RF-LH83020AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83020AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2RF-LH83020AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83030AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2RF-LH83030AI,17,17 Watts,1500,3000,120,120 Volt,103017649CHI-053 GB E2SF-LH83030AI with E2SFW-WW.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83030AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2RF-LH83030AI-277,17,17 Watts,1500,3000,277,277 Volt,103017649CHI-053 GB E2SF-LH83030AI with E2SFW-WW.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83040AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2RF-LH83040AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83040AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2RF-LH83040AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83060AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2RF-LH83060AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83060AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2RF-LH83060AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83520AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2RF-LH83520AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83520AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2RF-LH83520AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83530AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2RF-LH83530AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83530AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2RF-LH83530AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83540AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2RF-LH83540AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83540AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2RF-LH83540AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83560AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2RF-LH83560AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH83560AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2RF-LH83560AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,1,1,0,1
E2RF-LH92720AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2RF-LH92720AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH92720AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2RF-LH92720AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH92730AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2RF-LH92730AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH92730AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2RF-LH92730AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH92740AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2RF-LH92740AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH92740AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2RF-LH92740AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH92760AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2RF-LH92760AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH92760AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2RF-LH92760AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93020AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2RF-LH93020AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93020AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2RF-LH93020AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93030AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2RF-LH93030AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93030AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2RF-LH93030AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93040AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2RF-LH93040AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93040AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2RF-LH93040AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93060AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2RF-LH93060AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93060AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2RF-LH93060AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93520AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2RF-LH93520AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93520AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2RF-LH93520AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93530AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2RF-LH93530AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93530AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2RF-LH93530AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93540AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2RF-LH93540AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93540AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2RF-LH93540AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93560AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2RF-LH93560AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LH93560AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2RF-LH93560AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,1,1,0,1
E2RF-LO82720AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2RF-LO82720AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO82720AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2RF-LO82720AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO82730AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2RF-LO82730AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO82730AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2RF-LO82730AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO82740AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2RF-LO82740AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO82740AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2RF-LO82740AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO82760AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2RF-LO82760AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO82760AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2RF-LO82760AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83020AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2RF-LO83020AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83020AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2RF-LO83020AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83030AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2RF-LO83030AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83030AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2RF-LO83030AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83040AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2RF-LO83040AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83040AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2RF-LO83040AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83060AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2RF-LO83060AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83060AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2RF-LO83060AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83520AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2RF-LO83520AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83520AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2RF-LO83520AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83530AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2RF-LO83530AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83530AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2RF-LO83530AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83540AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2RF-LO83540AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83540AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2RF-LO83540AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83560AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2RF-LO83560AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO83560AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2RF-LO83560AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,1,0,1,1
E2RF-LO92720AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2RF-LO92720AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO92720AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2RF-LO92720AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO92730AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2RF-LO92730AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO92730AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2RF-LO92730AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO92740AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2RF-LO92740AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO92740AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2RF-LO92740AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO92760AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2RF-LO92760AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO92760AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2RF-LO92760AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93020AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2RF-LO93020AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93020AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2RF-LO93020AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93030AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2RF-LO93030AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93030AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2RF-LO93030AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93040AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2RF-LO93040AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93040AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2RF-LO93040AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93060AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2RF-LO93060AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93060AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2RF-LO93060AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93520AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2RF-LO93520AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93520AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2RF-LO93520AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93530AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2RF-LO93530AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93530AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2RF-LO93530AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93540AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2RF-LO93540AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93540AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2RF-LO93540AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93560AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2RF-LO93560AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO93560AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2RF-LO93560AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,1,0,1,1
E2RF-LO9WD20AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2RF-LO9WD20AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RF-LO9WD20AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2RF-LO9WD20AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RF-LO9WD30AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2RF-LO9WD30AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RF-LO9WD30AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2RF-LO9WD30AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RF-LO9WD40AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2RF-LO9WD40AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RF-LO9WD40AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2RF-LO9WD40AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RF-LO9WD60AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2RF-LO9WD60AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RF-LO9WD60AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2RF-LO9WD60AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,1,0,1,1
E2RT-LH82720AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2RT-LH82720AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH82720AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2RT-LH82720AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH82730AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2RT-LH82730AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH82730AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2RT-LH82730AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH82740AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2RT-LH82740AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH82740AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2RT-LH82740AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH82760AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2RT-LH82760AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH82760AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2RT-LH82760AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83020AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2RT-LH83020AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83020AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2RT-LH83020AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83030AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2RT-LH83030AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83030AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2RT-LH83030AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83040AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2RT-LH83040AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83040AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2RT-LH83040AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83060AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2RT-LH83060AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83060AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2RT-LH83060AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83520AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2RT-LH83520AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83520AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2RT-LH83520AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83530AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2RT-LH83530AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83530AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2RT-LH83530AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83540AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2RT-LH83540AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83540AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2RT-LH83540AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83560AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2RT-LH83560AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH83560AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2RT-LH83560AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,1,1,0,1
E2RT-LH92720AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2RT-LH92720AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH92720AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2RT-LH92720AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH92730AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2RT-LH92730AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH92730AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2RT-LH92730AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH92740AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2RT-LH92740AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH92740AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2RT-LH92740AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH92760AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2RT-LH92760AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH92760AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2RT-LH92760AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93020AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2RT-LH93020AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93020AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2RT-LH93020AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93030AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2RT-LH93030AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93030AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2RT-LH93030AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93040AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2RT-LH93040AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93040AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2RT-LH93040AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93060AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2RT-LH93060AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93060AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2RT-LH93060AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93520AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2RT-LH93520AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93520AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2RT-LH93520AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93530AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2RT-LH93530AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93530AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2RT-LH93530AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93540AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2RT-LH93540AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93540AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2RT-LH93540AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93560AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2RT-LH93560AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LH93560AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2RT-LH93560AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,1,1,0,1
E2RT-LO82720AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2RT-LO82720AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO82720AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2RT-LO82720AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO82730AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2RT-LO82730AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO82730AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2RT-LO82730AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO82740AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2RT-LO82740AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO82740AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2RT-LO82740AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO82760AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2RT-LO82760AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO82760AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2RT-LO82760AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83020AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2RT-LO83020AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83020AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2RT-LO83020AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83030AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2RT-LO83030AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83030AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2RT-LO83030AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83040AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2RT-LO83040AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83040AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2RT-LO83040AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83060AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2RT-LO83060AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83060AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2RT-LO83060AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83520AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2RT-LO83520AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83520AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2RT-LO83520AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83530AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2RT-LO83530AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83530AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2RT-LO83530AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83540AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2RT-LO83540AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83540AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2RT-LO83540AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83560AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2RT-LO83560AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO83560AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2RT-LO83560AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,1,0,1,1
E2RT-LO92720AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2RT-LO92720AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO92720AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2RT-LO92720AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO92730AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2RT-LO92730AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO92730AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2RT-LO92730AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO92740AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2RT-LO92740AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO92740AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2RT-LO92740AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO92760AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2RT-LO92760AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO92760AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2RT-LO92760AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93020AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2RT-LO93020AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93020AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2RT-LO93020AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93030AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2RT-LO93030AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93030AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2RT-LO93030AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93040AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2RT-LO93040AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93040AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2RT-LO93040AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93060AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2RT-LO93060AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93060AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2RT-LO93060AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93520AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2RT-LO93520AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93520AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2RT-LO93520AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93530AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2RT-LO93530AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93530AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2RT-LO93530AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93540AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2RT-LO93540AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93540AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2RT-LO93540AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93560AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2RT-LO93560AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO93560AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2RT-LO93560AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,1,0,1,1
E2RT-LO9WD20AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2RT-LO9WD20AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2RT-LO9WD20AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2RT-LO9WD20AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2RT-LO9WD30AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2RT-LO9WD30AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2RT-LO9WD30AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2RT-LO9WD30AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2RT-LO9WD40AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2RT-LO9WD40AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2RT-LO9WD40AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2RT-LO9WD40AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2RT-LO9WD60AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2RT-LO9WD60AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2RT-LO9WD60AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2RT-LO9WD60AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,1,0,1,1
E2SL-LH82720AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2SL-LH82720AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH82720AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2SL-LH82720AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH82730AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2SL-LH82730AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH82730AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2SL-LH82730AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH82740AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2SL-LH82740AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH82740AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2SL-LH82740AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH82760AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2SL-LH82760AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH82760AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2SL-LH82760AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83020AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2SL-LH83020AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83020AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2SL-LH83020AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83030AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2SL-LH83030AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83030AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2SL-LH83030AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83040AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2SL-LH83040AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83040AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2SL-LH83040AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83060AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2SL-LH83060AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83060AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2SL-LH83060AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83520AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2SL-LH83520AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83520AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2SL-LH83520AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83530AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2SL-LH83530AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83530AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2SL-LH83530AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83540AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2SL-LH83540AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83540AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2SL-LH83540AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83560AI,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2SL-LH83560AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH83560AI-277,Flangeless (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2SL-LH83560AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,0
E2SL-LH92720AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2SL-LH92720AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH92720AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2SL-LH92720AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH92730AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2SL-LH92730AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH92730AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2SL-LH92730AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH92740AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2SL-LH92740AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH92740AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2SL-LH92740AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH92760AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2SL-LH92760AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH92760AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2SL-LH92760AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93020AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2SL-LH93020AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93020AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2SL-LH93020AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93030AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2SL-LH93030AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93030AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2SL-LH93030AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93040AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2SL-LH93040AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93040AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2SL-LH93040AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93060AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2SL-LH93060AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93060AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2SL-LH93060AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93520AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2SL-LH93520AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93520AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2SL-LH93520AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93530AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2SL-LH93530AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93530AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2SL-LH93530AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93540AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2SL-LH93540AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93540AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2SL-LH93540AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93560AI,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2SL-LH93560AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LH93560AI-277,Flangeless (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2SL-LH93560AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,0
E2SL-LO82720AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2SL-LO82720AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO82720AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2SL-LO82720AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO82730AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2SL-LO82730AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO82730AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2SL-LO82730AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO82740AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2SL-LO82740AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO82740AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2SL-LO82740AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO82760AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2SL-LO82760AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO82760AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2SL-LO82760AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83020AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2SL-LO83020AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83020AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2SL-LO83020AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83030AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2SL-LO83030AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83030AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2SL-LO83030AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83040AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2SL-LO83040AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83040AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2SL-LO83040AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83060AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2SL-LO83060AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83060AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2SL-LO83060AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83520AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2SL-LO83520AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83520AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2SL-LO83520AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83530AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2SL-LO83530AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83530AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2SL-LO83530AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83540AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2SL-LO83540AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83540AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2SL-LO83540AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83560AI,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2SL-LO83560AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO83560AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2SL-LO83560AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,0
E2SL-LO92720AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2SL-LO92720AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO92720AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2SL-LO92720AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO92730AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2SL-LO92730AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO92730AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2SL-LO92730AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO92740AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2SL-LO92740AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO92740AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2SL-LO92740AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO92760AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2SL-LO92760AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO92760AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2SL-LO92760AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93020AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2SL-LO93020AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93020AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2SL-LO93020AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93030AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2SL-LO93030AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93030AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2SL-LO93030AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93040AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2SL-LO93040AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93040AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2SL-LO93040AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93060AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2SL-LO93060AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93060AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2SL-LO93060AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93520AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2SL-LO93520AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93520AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2SL-LO93520AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93530AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2SL-LO93530AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93530AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2SL-LO93530AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93540AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2SL-LO93540AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93540AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2SL-LO93540AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93560AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2SL-LO93560AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO93560AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2SL-LO93560AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,0
E2SL-LO9WD20AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2SL-LO9WD20AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SL-LO9WD20AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2SL-LO9WD20AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SL-LO9WD30AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2SL-LO9WD30AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SL-LO9WD30AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2SL-LO9WD30AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SL-LO9WD40AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2SL-LO9WD40AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SL-LO9WD40AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2SL-LO9WD40AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SL-LO9WD60AI,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2SL-LO9WD60AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SL-LO9WD60AI-277,Flangeless (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2SL-LO9WD60AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,0
E2SF-LH82720AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2SF-LH82720AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH82720AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2SF-LH82720AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH82730AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2SF-LH82730AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH82730AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2SF-LH82730AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH82740AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2SF-LH82740AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH82740AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2SF-LH82740AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH82760AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2SF-LH82760AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH82760AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2SF-LH82760AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83020AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2SF-LH83020AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83020AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2SF-LH83020AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83030AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2SF-LH83030AI,17,17 Watts,1500,3000,120,120 Volt,103017649CHI-053 GB E2SF-LH83030AI with E2SFW-WW.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83030AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2SF-LH83030AI-277,17,17 Watts,1500,3000,277,277 Volt,103017649CHI-053 GB E2SF-LH83030AI with E2SFW-WW.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83040AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2SF-LH83040AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83040AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2SF-LH83040AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83060AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2SF-LH83060AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83060AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2SF-LH83060AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83520AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2SF-LH83520AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83520AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2SF-LH83520AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83530AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2SF-LH83530AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83530AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2SF-LH83530AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83540AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2SF-LH83540AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83540AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2SF-LH83540AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83560AI,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2SF-LH83560AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH83560AI-277,Flanged (Ceiling Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2SF-LH83560AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,88,17,2,1,0,1
E2SF-LH92720AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2SF-LH92720AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH92720AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2SF-LH92720AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH92730AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2SF-LH92730AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH92730AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2SF-LH92730AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH92740AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2SF-LH92740AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH92740AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2SF-LH92740AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH92760AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2SF-LH92760AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH92760AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2SF-LH92760AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93020AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2SF-LH93020AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93020AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2SF-LH93020AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93030AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2SF-LH93030AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93030AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2SF-LH93030AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93040AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2SF-LH93040AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93040AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2SF-LH93040AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93060AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2SF-LH93060AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93060AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2SF-LH93060AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93520AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2SF-LH93520AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93520AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2SF-LH93520AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93530AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2SF-LH93530AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93530AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2SF-LH93530AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93540AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2SF-LH93540AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93540AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2SF-LH93540AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93560AI,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2SF-LH93560AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LH93560AI-277,Flanged (Ceiling Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2SF-LH93560AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,73,17,2,1,0,1
E2SF-LO82720AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2SF-LO82720AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO82720AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2SF-LO82720AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO82730AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2SF-LO82730AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO82730AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2SF-LO82730AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO82740AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2SF-LO82740AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO82740AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2SF-LO82740AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO82760AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2SF-LO82760AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO82760AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2SF-LO82760AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83020AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2SF-LO83020AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83020AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2SF-LO83020AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83030AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2SF-LO83030AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83030AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2SF-LO83030AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83040AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2SF-LO83040AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83040AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2SF-LO83040AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83060AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2SF-LO83060AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83060AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2SF-LO83060AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83520AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2SF-LO83520AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83520AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2SF-LO83520AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83530AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2SF-LO83530AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83530AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2SF-LO83530AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83540AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2SF-LO83540AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83540AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2SF-LO83540AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83560AI,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2SF-LO83560AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO83560AI-277,Flanged (Ceiling Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2SF-LO83560AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,97,12,2,0,1,1
E2SF-LO92720AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2SF-LO92720AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO92720AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2SF-LO92720AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO92730AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2SF-LO92730AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO92730AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2SF-LO92730AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO92740AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2SF-LO92740AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO92740AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2SF-LO92740AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO92760AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2SF-LO92760AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO92760AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2SF-LO92760AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93020AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2SF-LO93020AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93020AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2SF-LO93020AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93030AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2SF-LO93030AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93030AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2SF-LO93030AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93040AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2SF-LO93040AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93040AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2SF-LO93040AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93060AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2SF-LO93060AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93060AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2SF-LO93060AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93520AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2SF-LO93520AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93520AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2SF-LO93520AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93530AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2SF-LO93530AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93530AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2SF-LO93530AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93540AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2SF-LO93540AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93540AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2SF-LO93540AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93560AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2SF-LO93560AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO93560AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2SF-LO93560AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,77,12,2,0,1,1
E2SF-LO9WD20AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2SF-LO9WD20AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2SF-LO9WD20AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2SF-LO9WD20AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2SF-LO9WD30AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2SF-LO9WD30AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2SF-LO9WD30AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2SF-LO9WD30AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2SF-LO9WD40AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2SF-LO9WD40AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2SF-LO9WD40AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2SF-LO9WD40AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2SF-LO9WD60AI,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2SF-LO9WD60AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2SF-LO9WD60AI-277,Flanged (Ceiling Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2SF-LO9WD60AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2.pdf,71,12,2,0,1,1
E2ST-LH82720AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2ST-LH82720AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH82720AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",20°,IC Airtight,E2ST-LH82720AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH82730AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2ST-LH82730AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH82730AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",30°,IC Airtight,E2ST-LH82730AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH82740AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2ST-LH82740AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH82740AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",40°,IC Airtight,E2ST-LH82740AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH82760AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2ST-LH82760AI,17,17 Watts,1500,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH82760AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 2700K",60°,IC Airtight,E2ST-LH82760AI-277,17,17 Watts,1500,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83020AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2ST-LH83020AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83020AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",20°,IC Airtight,E2ST-LH83020AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83030AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2ST-LH83030AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83030AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",30°,IC Airtight,E2ST-LH83030AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83040AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2ST-LH83040AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83040AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",40°,IC Airtight,E2ST-LH83040AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83060AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2ST-LH83060AI,17,17 Watts,1500,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83060AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3000K",60°,IC Airtight,E2ST-LH83060AI-277,17,17 Watts,1500,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83520AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2ST-LH83520AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83520AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",20°,IC Airtight,E2ST-LH83520AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83530AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2ST-LH83530AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83530AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",30°,IC Airtight,E2ST-LH83530AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83540AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2ST-LH83540AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83540AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",40°,IC Airtight,E2ST-LH83540AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83560AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2ST-LH83560AI,17,17 Watts,1500,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH83560AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","80 CRI, 3500K",60°,IC Airtight,E2ST-LH83560AI-277,17,17 Watts,1500,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,88,17,2,1,0,1
E2ST-LH92720AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2ST-LH92720AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH92720AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",20°,IC Airtight,E2ST-LH92720AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH92730AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2ST-LH92730AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH92730AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",30°,IC Airtight,E2ST-LH92730AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH92740AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2ST-LH92740AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH92740AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",40°,IC Airtight,E2ST-LH92740AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH92760AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2ST-LH92760AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH92760AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 2700K",60°,IC Airtight,E2ST-LH92760AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93020AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2ST-LH93020AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93020AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",20°,IC Airtight,E2ST-LH93020AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93030AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2ST-LH93030AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93030AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",30°,IC Airtight,E2ST-LH93030AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93040AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2ST-LH93040AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93040AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",40°,IC Airtight,E2ST-LH93040AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93060AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2ST-LH93060AI,17,17 Watts,1250,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93060AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3000K",60°,IC Airtight,E2ST-LH93060AI-277,17,17 Watts,1250,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93520AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2ST-LH93520AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93520AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",20°,IC Airtight,E2ST-LH93520AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93530AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2ST-LH93530AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93530AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",30°,IC Airtight,E2ST-LH93530AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93540AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2ST-LH93540AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93540AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",40°,IC Airtight,E2ST-LH93540AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93560AI,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2ST-LH93560AI,17,17 Watts,1250,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LH93560AI-277,T-Grid/Flanged (Housing Mount),"High Output , 17W","90 CRI, 3500K",60°,IC Airtight,E2ST-LH93560AI-277,17,17 Watts,1250,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,73,17,2,1,0,1
E2ST-LO82720AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2ST-LO82720AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO82720AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",20°,IC Airtight,E2ST-LO82720AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO82730AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2ST-LO82730AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO82730AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",30°,IC Airtight,E2ST-LO82730AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO82740AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2ST-LO82740AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO82740AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",40°,IC Airtight,E2ST-LO82740AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO82760AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2ST-LO82760AI,12,12 Watts,1163,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO82760AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 2700K",60°,IC Airtight,E2ST-LO82760AI-277,12,12 Watts,1163,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83020AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2ST-LO83020AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83020AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",20°,IC Airtight,E2ST-LO83020AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83030AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2ST-LO83030AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83030AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",30°,IC Airtight,E2ST-LO83030AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83040AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2ST-LO83040AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83040AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",40°,IC Airtight,E2ST-LO83040AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83060AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2ST-LO83060AI,12,12 Watts,1163,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83060AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3000K",60°,IC Airtight,E2ST-LO83060AI-277,12,12 Watts,1163,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83520AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2ST-LO83520AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83520AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",20°,IC Airtight,E2ST-LO83520AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83530AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2ST-LO83530AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83530AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",30°,IC Airtight,E2ST-LO83530AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83540AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2ST-LO83540AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83540AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",40°,IC Airtight,E2ST-LO83540AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83560AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2ST-LO83560AI,12,12 Watts,1163,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO83560AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","80 CRI, 3500K",60°,IC Airtight,E2ST-LO83560AI-277,12,12 Watts,1163,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,97,12,2,0,1,1
E2ST-LO92720AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2ST-LO92720AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO92720AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",20°,IC Airtight,E2ST-LO92720AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO92730AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2ST-LO92730AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO92730AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",30°,IC Airtight,E2ST-LO92730AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO92740AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2ST-LO92740AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO92740AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",40°,IC Airtight,E2ST-LO92740AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO92760AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2ST-LO92760AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO92760AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 2700K",60°,IC Airtight,E2ST-LO92760AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93020AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2ST-LO93020AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93020AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",20°,IC Airtight,E2ST-LO93020AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93030AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2ST-LO93030AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93030AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",30°,IC Airtight,E2ST-LO93030AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93040AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2ST-LO93040AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93040AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",40°,IC Airtight,E2ST-LO93040AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93060AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2ST-LO93060AI,12,12 Watts,930,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93060AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3000K",60°,IC Airtight,E2ST-LO93060AI-277,12,12 Watts,930,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93520AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2ST-LO93520AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93520AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",20°,IC Airtight,E2ST-LO93520AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93530AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2ST-LO93530AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93530AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",30°,IC Airtight,E2ST-LO93530AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93540AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2ST-LO93540AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93540AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",40°,IC Airtight,E2ST-LO93540AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93560AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2ST-LO93560AI,12,12 Watts,930,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO93560AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, 3500K",60°,IC Airtight,E2ST-LO93560AI-277,12,12 Watts,930,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,77,12,2,0,1,1
E2ST-LO9WD20AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2ST-LO9WD20AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
E2ST-LO9WD20AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",20°,IC Airtight,E2ST-LO9WD20AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
E2ST-LO9WD30AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2ST-LO9WD30AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
E2ST-LO9WD30AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",30°,IC Airtight,E2ST-LO9WD30AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
E2ST-LO9WD40AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2ST-LO9WD40AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
E2ST-LO9WD40AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",40°,IC Airtight,E2ST-LO9WD40AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
E2ST-LO9WD60AI,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2ST-LO9WD60AI,12,12 Watts,850,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
E2ST-LO9WD60AI-277,T-Grid/Flanged (Housing Mount),"Low Output, 12W","90 CRI, Warm Dim",60°,IC Airtight,E2ST-LO9WD60AI-277,12,12 Watts,850,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E2T.pdf,71,12,2,0,1,1
