,Model##other##,Product (Housing)##other##,Ceiling Appearance (Housing)##other##,Output (Housing)##other##,Driver (Housing)##other##,Product (Trim)##other##,Ceiling Appearance (Trim)##other##,Style (Trim)##other##,Function (Trim)##other##,LED (Trim)##other##,Beam Spread (Trim)##other##,Finish (Trim)##other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Wattage Comments##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Photometric Web File##OTHER##,Constraints##other##,Constraints Ceiling##other##,Finish##other##
E3RF-LHIMUNV E3RFBD92218-BM,E3RF-LHIMUNV E3RFBD92218-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92218-NBM,E3RF-LHIMUNV E3RFBD92218-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92218-WM,E3RF-LHIMUNV E3RFBD92218-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92418-BM,E3RF-LHIMUNV E3RFBD92418-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92418-NBM,E3RF-LHIMUNV E3RFBD92418-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92418-WM,E3RF-LHIMUNV E3RFBD92418-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92718-BM,E3RF-LHIMUNV E3RFBD92718-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92718-NBM,E3RF-LHIMUNV E3RFBD92718-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92718-WM,E3RF-LHIMUNV E3RFBD92718-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93018-BM,E3RF-LHIMUNV E3RFBD93018-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93018-NBM,E3RF-LHIMUNV E3RFBD93018-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93018-WM,E3RF-LHIMUNV E3RFBD93018-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93518-BM,E3RF-LHIMUNV E3RFBD93518-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93518-NBM,E3RF-LHIMUNV E3RFBD93518-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93518-WM,E3RF-LHIMUNV E3RFBD93518-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD9WD18-BM,E3RF-LHIMUNV E3RFBD9WD18-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD9WD18-NBM,E3RF-LHIMUNV E3RFBD9WD18-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD9WD18-WM,E3RF-LHIMUNV E3RFBD9WD18-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92225-BM,E3RF-LHIMUNV E3RFBD92225-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92225-NBM,E3RF-LHIMUNV E3RFBD92225-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92225-WM,E3RF-LHIMUNV E3RFBD92225-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92425-BM,E3RF-LHIMUNV E3RFBD92425-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92425-NBM,E3RF-LHIMUNV E3RFBD92425-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92425-WM,E3RF-LHIMUNV E3RFBD92425-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92725-BM,E3RF-LHIMUNV E3RFBD92725-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92725-NBM,E3RF-LHIMUNV E3RFBD92725-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92725-WM,E3RF-LHIMUNV E3RFBD92725-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93025-BM,E3RF-LHIMUNV E3RFBD93025-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93025-NBM,E3RF-LHIMUNV E3RFBD93025-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93025-WM,E3RF-LHIMUNV E3RFBD93025-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93525-BM,E3RF-LHIMUNV E3RFBD93525-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93525-NBM,E3RF-LHIMUNV E3RFBD93525-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93525-WM,E3RF-LHIMUNV E3RFBD93525-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD9WD25-BM,E3RF-LHIMUNV E3RFBD9WD25-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD9WD25-NBM,E3RF-LHIMUNV E3RFBD9WD25-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD9WD25-WM,E3RF-LHIMUNV E3RFBD9WD25-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92240-BM,E3RF-LHIMUNV E3RFBD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92240-NBM,E3RF-LHIMUNV E3RFBD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92240-WM,E3RF-LHIMUNV E3RFBD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92440-BM,E3RF-LHIMUNV E3RFBD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92440-NBM,E3RF-LHIMUNV E3RFBD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92440-WM,E3RF-LHIMUNV E3RFBD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92740-BM,E3RF-LHIMUNV E3RFBD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92740-NBM,E3RF-LHIMUNV E3RFBD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92740-WM,E3RF-LHIMUNV E3RFBD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93040-BM,E3RF-LHIMUNV E3RFBD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93040-NBM,E3RF-LHIMUNV E3RFBD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93040-WM,E3RF-LHIMUNV E3RFBD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93540-BM,E3RF-LHIMUNV E3RFBD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93540-NBM,E3RF-LHIMUNV E3RFBD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93540-WM,E3RF-LHIMUNV E3RFBD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD9WD40-BM,E3RF-LHIMUNV E3RFBD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD9WD40-NBM,E3RF-LHIMUNV E3RFBD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD9WD40-WM,E3RF-LHIMUNV E3RFBD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RFBD92240-BM,E3RF-LOIMUNV E3RFBD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RFBD92240-NBM,E3RF-LOIMUNV E3RFBD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RFBD92240-WM,E3RF-LOIMUNV E3RFBD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RFBD92440-BM,E3RF-LOIMUNV E3RFBD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RFBD92440-NBM,E3RF-LOIMUNV E3RFBD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RFBD92440-WM,E3RF-LOIMUNV E3RFBD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RFBD92740-BM,E3RF-LOIMUNV E3RFBD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RFBD92740-NBM,E3RF-LOIMUNV E3RFBD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RFBD92740-WM,E3RF-LOIMUNV E3RFBD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RFBD93040-BM,E3RF-LOIMUNV E3RFBD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RFBD93040-NBM,E3RF-LOIMUNV E3RFBD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RFBD93040-WM,E3RF-LOIMUNV E3RFBD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RFBD93540-BM,E3RF-LOIMUNV E3RFBD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RFBD93540-NBM,E3RF-LOIMUNV E3RFBD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RFBD93540-WM,E3RF-LOIMUNV E3RFBD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RFBD9WD40-BM,E3RF-LOIMUNV E3RFBD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RFBD9WD40-NBM,E3RF-LOIMUNV E3RFBD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RFBD9WD40-WM,E3RF-LOIMUNV E3RFBD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92260-BM,E3RF-LHIMUNV E3RFBD92260-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92260-NBM,E3RF-LHIMUNV E3RFBD92260-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92260-WM,E3RF-LHIMUNV E3RFBD92260-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92460-BM,E3RF-LHIMUNV E3RFBD92460-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92460-NBM,E3RF-LHIMUNV E3RFBD92460-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92460-WM,E3RF-LHIMUNV E3RFBD92460-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD92760-BM,E3RF-LHIMUNV E3RFBD92760-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD92760-NBM,E3RF-LHIMUNV E3RFBD92760-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD92760-WM,E3RF-LHIMUNV E3RFBD92760-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93060-BM,E3RF-LHIMUNV E3RFBD93060-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93060-NBM,E3RF-LHIMUNV E3RFBD93060-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93060-WM,E3RF-LHIMUNV E3RFBD93060-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD93560-BM,E3RF-LHIMUNV E3RFBD93560-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD93560-NBM,E3RF-LHIMUNV E3RFBD93560-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD93560-WM,E3RF-LHIMUNV E3RFBD93560-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RFBD9WD60-BM,E3RF-LHIMUNV E3RFBD9WD60-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,1,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RFBD9WD60-NBM,E3RF-LHIMUNV E3RFBD9WD60-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,1,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RFBD9WD60-WM,E3RF-LHIMUNV E3RFBD9WD60-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,1,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92218-BM,E3RF-LHIMUNV E3RF15BD92218-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92218-NBM,E3RF-LHIMUNV E3RF15BD92218-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92218-WM,E3RF-LHIMUNV E3RF15BD92218-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92418-BM,E3RF-LHIMUNV E3RF15BD92418-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92418-NBM,E3RF-LHIMUNV E3RF15BD92418-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92418-WM,E3RF-LHIMUNV E3RF15BD92418-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92718-BM,E3RF-LHIMUNV E3RF15BD92718-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92718-NBM,E3RF-LHIMUNV E3RF15BD92718-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92718-WM,E3RF-LHIMUNV E3RF15BD92718-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93018-BM,E3RF-LHIMUNV E3RF15BD93018-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93018-NBM,E3RF-LHIMUNV E3RF15BD93018-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93018-WM,E3RF-LHIMUNV E3RF15BD93018-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93518-BM,E3RF-LHIMUNV E3RF15BD93518-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93518-NBM,E3RF-LHIMUNV E3RF15BD93518-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93518-WM,E3RF-LHIMUNV E3RF15BD93518-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD9WD18-BM,E3RF-LHIMUNV E3RF15BD9WD18-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD9WD18-NBM,E3RF-LHIMUNV E3RF15BD9WD18-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD9WD18-WM,E3RF-LHIMUNV E3RF15BD9WD18-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92225-BM,E3RF-LHIMUNV E3RF15BD92225-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92225-NBM,E3RF-LHIMUNV E3RF15BD92225-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92225-WM,E3RF-LHIMUNV E3RF15BD92225-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92425-BM,E3RF-LHIMUNV E3RF15BD92425-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92425-NBM,E3RF-LHIMUNV E3RF15BD92425-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92425-WM,E3RF-LHIMUNV E3RF15BD92425-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92725-BM,E3RF-LHIMUNV E3RF15BD92725-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92725-NBM,E3RF-LHIMUNV E3RF15BD92725-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92725-WM,E3RF-LHIMUNV E3RF15BD92725-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93025-BM,E3RF-LHIMUNV E3RF15BD93025-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93025-NBM,E3RF-LHIMUNV E3RF15BD93025-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93025-WM,E3RF-LHIMUNV E3RF15BD93025-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93525-BM,E3RF-LHIMUNV E3RF15BD93525-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93525-NBM,E3RF-LHIMUNV E3RF15BD93525-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93525-WM,E3RF-LHIMUNV E3RF15BD93525-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD9WD25-BM,E3RF-LHIMUNV E3RF15BD9WD25-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD9WD25-NBM,E3RF-LHIMUNV E3RF15BD9WD25-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD9WD25-WM,E3RF-LHIMUNV E3RF15BD9WD25-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92240-BM,E3RF-LHIMUNV E3RF15BD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92240-NBM,E3RF-LHIMUNV E3RF15BD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92240-WM,E3RF-LHIMUNV E3RF15BD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92440-BM,E3RF-LHIMUNV E3RF15BD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92440-NBM,E3RF-LHIMUNV E3RF15BD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92440-WM,E3RF-LHIMUNV E3RF15BD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92740-BM,E3RF-LHIMUNV E3RF15BD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92740-NBM,E3RF-LHIMUNV E3RF15BD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92740-WM,E3RF-LHIMUNV E3RF15BD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93040-BM,E3RF-LHIMUNV E3RF15BD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93040-NBM,E3RF-LHIMUNV E3RF15BD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93040-WM,E3RF-LHIMUNV E3RF15BD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93540-BM,E3RF-LHIMUNV E3RF15BD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93540-NBM,E3RF-LHIMUNV E3RF15BD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93540-WM,E3RF-LHIMUNV E3RF15BD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD9WD40-BM,E3RF-LHIMUNV E3RF15BD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD9WD40-NBM,E3RF-LHIMUNV E3RF15BD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD9WD40-WM,E3RF-LHIMUNV E3RF15BD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF15BD92240-BM,E3RF-LOIMUNV E3RF15BD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF15BD92240-NBM,E3RF-LOIMUNV E3RF15BD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF15BD92240-WM,E3RF-LOIMUNV E3RF15BD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF15BD92440-BM,E3RF-LOIMUNV E3RF15BD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF15BD92440-NBM,E3RF-LOIMUNV E3RF15BD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF15BD92440-WM,E3RF-LOIMUNV E3RF15BD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF15BD92740-BM,E3RF-LOIMUNV E3RF15BD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF15BD92740-NBM,E3RF-LOIMUNV E3RF15BD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF15BD92740-WM,E3RF-LOIMUNV E3RF15BD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF15BD93040-BM,E3RF-LOIMUNV E3RF15BD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF15BD93040-NBM,E3RF-LOIMUNV E3RF15BD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF15BD93040-WM,E3RF-LOIMUNV E3RF15BD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF15BD93540-BM,E3RF-LOIMUNV E3RF15BD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF15BD93540-NBM,E3RF-LOIMUNV E3RF15BD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF15BD93540-WM,E3RF-LOIMUNV E3RF15BD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF15BD9WD40-BM,E3RF-LOIMUNV E3RF15BD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF15BD9WD40-NBM,E3RF-LOIMUNV E3RF15BD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF15BD9WD40-WM,E3RF-LOIMUNV E3RF15BD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92260-BM,E3RF-LHIMUNV E3RF15BD92260-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92260-NBM,E3RF-LHIMUNV E3RF15BD92260-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92260-WM,E3RF-LHIMUNV E3RF15BD92260-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92460-BM,E3RF-LHIMUNV E3RF15BD92460-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92460-NBM,E3RF-LHIMUNV E3RF15BD92460-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92460-WM,E3RF-LHIMUNV E3RF15BD92460-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD92760-BM,E3RF-LHIMUNV E3RF15BD92760-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD92760-NBM,E3RF-LHIMUNV E3RF15BD92760-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD92760-WM,E3RF-LHIMUNV E3RF15BD92760-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93060-BM,E3RF-LHIMUNV E3RF15BD93060-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93060-NBM,E3RF-LHIMUNV E3RF15BD93060-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93060-WM,E3RF-LHIMUNV E3RF15BD93060-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD93560-BM,E3RF-LHIMUNV E3RF15BD93560-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD93560-NBM,E3RF-LHIMUNV E3RF15BD93560-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD93560-WM,E3RF-LHIMUNV E3RF15BD93560-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF15BD9WD60-BM,E3RF-LHIMUNV E3RF15BD9WD60-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,2,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF15BD9WD60-NBM,E3RF-LHIMUNV E3RF15BD9WD60-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,2,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF15BD9WD60-WM,E3RF-LHIMUNV E3RF15BD9WD60-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,2,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92218-BM,E3RF-LHIMUNV E3RF20BD92218-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92218-NBM,E3RF-LHIMUNV E3RF20BD92218-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92218-WM,E3RF-LHIMUNV E3RF20BD92218-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92418-BM,E3RF-LHIMUNV E3RF20BD92418-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92418-NBM,E3RF-LHIMUNV E3RF20BD92418-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92418-WM,E3RF-LHIMUNV E3RF20BD92418-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92718-BM,E3RF-LHIMUNV E3RF20BD92718-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92718-NBM,E3RF-LHIMUNV E3RF20BD92718-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92718-WM,E3RF-LHIMUNV E3RF20BD92718-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93018-BM,E3RF-LHIMUNV E3RF20BD93018-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93018-NBM,E3RF-LHIMUNV E3RF20BD93018-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93018-WM,E3RF-LHIMUNV E3RF20BD93018-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93518-BM,E3RF-LHIMUNV E3RF20BD93518-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93518-NBM,E3RF-LHIMUNV E3RF20BD93518-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93518-WM,E3RF-LHIMUNV E3RF20BD93518-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD9WD18-BM,E3RF-LHIMUNV E3RF20BD9WD18-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD9WD18-NBM,E3RF-LHIMUNV E3RF20BD9WD18-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD9WD18-WM,E3RF-LHIMUNV E3RF20BD9WD18-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92225-BM,E3RF-LHIMUNV E3RF20BD92225-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92225-NBM,E3RF-LHIMUNV E3RF20BD92225-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92225-WM,E3RF-LHIMUNV E3RF20BD92225-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92425-BM,E3RF-LHIMUNV E3RF20BD92425-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92425-NBM,E3RF-LHIMUNV E3RF20BD92425-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92425-WM,E3RF-LHIMUNV E3RF20BD92425-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92725-BM,E3RF-LHIMUNV E3RF20BD92725-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92725-NBM,E3RF-LHIMUNV E3RF20BD92725-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92725-WM,E3RF-LHIMUNV E3RF20BD92725-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93025-BM,E3RF-LHIMUNV E3RF20BD93025-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93025-NBM,E3RF-LHIMUNV E3RF20BD93025-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93025-WM,E3RF-LHIMUNV E3RF20BD93025-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93525-BM,E3RF-LHIMUNV E3RF20BD93525-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93525-NBM,E3RF-LHIMUNV E3RF20BD93525-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93525-WM,E3RF-LHIMUNV E3RF20BD93525-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD9WD25-BM,E3RF-LHIMUNV E3RF20BD9WD25-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD9WD25-NBM,E3RF-LHIMUNV E3RF20BD9WD25-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD9WD25-WM,E3RF-LHIMUNV E3RF20BD9WD25-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92240-BM,E3RF-LHIMUNV E3RF20BD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92240-NBM,E3RF-LHIMUNV E3RF20BD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92240-WM,E3RF-LHIMUNV E3RF20BD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92440-BM,E3RF-LHIMUNV E3RF20BD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92440-NBM,E3RF-LHIMUNV E3RF20BD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92440-WM,E3RF-LHIMUNV E3RF20BD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92740-BM,E3RF-LHIMUNV E3RF20BD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92740-NBM,E3RF-LHIMUNV E3RF20BD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92740-WM,E3RF-LHIMUNV E3RF20BD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93040-BM,E3RF-LHIMUNV E3RF20BD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93040-NBM,E3RF-LHIMUNV E3RF20BD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93040-WM,E3RF-LHIMUNV E3RF20BD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93540-BM,E3RF-LHIMUNV E3RF20BD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93540-NBM,E3RF-LHIMUNV E3RF20BD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93540-WM,E3RF-LHIMUNV E3RF20BD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD9WD40-BM,E3RF-LHIMUNV E3RF20BD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD9WD40-NBM,E3RF-LHIMUNV E3RF20BD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD9WD40-WM,E3RF-LHIMUNV E3RF20BD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF20BD92240-BM,E3RF-LOIMUNV E3RF20BD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF20BD92240-NBM,E3RF-LOIMUNV E3RF20BD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF20BD92240-WM,E3RF-LOIMUNV E3RF20BD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF20BD92440-BM,E3RF-LOIMUNV E3RF20BD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF20BD92440-NBM,E3RF-LOIMUNV E3RF20BD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF20BD92440-WM,E3RF-LOIMUNV E3RF20BD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF20BD92740-BM,E3RF-LOIMUNV E3RF20BD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF20BD92740-NBM,E3RF-LOIMUNV E3RF20BD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF20BD92740-WM,E3RF-LOIMUNV E3RF20BD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF20BD93040-BM,E3RF-LOIMUNV E3RF20BD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF20BD93040-NBM,E3RF-LOIMUNV E3RF20BD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF20BD93040-WM,E3RF-LOIMUNV E3RF20BD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF20BD93540-BM,E3RF-LOIMUNV E3RF20BD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF20BD93540-NBM,E3RF-LOIMUNV E3RF20BD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF20BD93540-WM,E3RF-LOIMUNV E3RF20BD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF20BD9WD40-BM,E3RF-LOIMUNV E3RF20BD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF20BD9WD40-NBM,E3RF-LOIMUNV E3RF20BD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF20BD9WD40-WM,E3RF-LOIMUNV E3RF20BD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92260-BM,E3RF-LHIMUNV E3RF20BD92260-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92260-NBM,E3RF-LHIMUNV E3RF20BD92260-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92260-WM,E3RF-LHIMUNV E3RF20BD92260-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92460-BM,E3RF-LHIMUNV E3RF20BD92460-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92460-NBM,E3RF-LHIMUNV E3RF20BD92460-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92460-WM,E3RF-LHIMUNV E3RF20BD92460-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD92760-BM,E3RF-LHIMUNV E3RF20BD92760-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD92760-NBM,E3RF-LHIMUNV E3RF20BD92760-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD92760-WM,E3RF-LHIMUNV E3RF20BD92760-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93060-BM,E3RF-LHIMUNV E3RF20BD93060-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93060-NBM,E3RF-LHIMUNV E3RF20BD93060-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93060-WM,E3RF-LHIMUNV E3RF20BD93060-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD93560-BM,E3RF-LHIMUNV E3RF20BD93560-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD93560-NBM,E3RF-LHIMUNV E3RF20BD93560-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD93560-WM,E3RF-LHIMUNV E3RF20BD93560-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF20BD9WD60-BM,E3RF-LHIMUNV E3RF20BD9WD60-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,3,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF20BD9WD60-NBM,E3RF-LHIMUNV E3RF20BD9WD60-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,3,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF20BD9WD60-WM,E3RF-LHIMUNV E3RF20BD9WD60-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,3,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92218-BM,E3RF-LHIMUNV E3RF25BD92218-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92218-NBM,E3RF-LHIMUNV E3RF25BD92218-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92218-WM,E3RF-LHIMUNV E3RF25BD92218-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92418-BM,E3RF-LHIMUNV E3RF25BD92418-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92418-NBM,E3RF-LHIMUNV E3RF25BD92418-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92418-WM,E3RF-LHIMUNV E3RF25BD92418-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92718-BM,E3RF-LHIMUNV E3RF25BD92718-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92718-NBM,E3RF-LHIMUNV E3RF25BD92718-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92718-WM,E3RF-LHIMUNV E3RF25BD92718-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93018-BM,E3RF-LHIMUNV E3RF25BD93018-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93018-NBM,E3RF-LHIMUNV E3RF25BD93018-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93018-WM,E3RF-LHIMUNV E3RF25BD93018-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93518-BM,E3RF-LHIMUNV E3RF25BD93518-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93518-NBM,E3RF-LHIMUNV E3RF25BD93518-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93518-WM,E3RF-LHIMUNV E3RF25BD93518-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD9WD18-BM,E3RF-LHIMUNV E3RF25BD9WD18-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD9WD18-NBM,E3RF-LHIMUNV E3RF25BD9WD18-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD9WD18-WM,E3RF-LHIMUNV E3RF25BD9WD18-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92225-BM,E3RF-LHIMUNV E3RF25BD92225-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92225-NBM,E3RF-LHIMUNV E3RF25BD92225-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92225-WM,E3RF-LHIMUNV E3RF25BD92225-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92425-BM,E3RF-LHIMUNV E3RF25BD92425-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92425-NBM,E3RF-LHIMUNV E3RF25BD92425-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92425-WM,E3RF-LHIMUNV E3RF25BD92425-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92725-BM,E3RF-LHIMUNV E3RF25BD92725-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92725-NBM,E3RF-LHIMUNV E3RF25BD92725-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92725-WM,E3RF-LHIMUNV E3RF25BD92725-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93025-BM,E3RF-LHIMUNV E3RF25BD93025-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93025-NBM,E3RF-LHIMUNV E3RF25BD93025-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93025-WM,E3RF-LHIMUNV E3RF25BD93025-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93525-BM,E3RF-LHIMUNV E3RF25BD93525-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93525-NBM,E3RF-LHIMUNV E3RF25BD93525-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93525-WM,E3RF-LHIMUNV E3RF25BD93525-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD9WD25-BM,E3RF-LHIMUNV E3RF25BD9WD25-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD9WD25-NBM,E3RF-LHIMUNV E3RF25BD9WD25-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD9WD25-WM,E3RF-LHIMUNV E3RF25BD9WD25-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92240-BM,E3RF-LHIMUNV E3RF25BD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92240-NBM,E3RF-LHIMUNV E3RF25BD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92240-WM,E3RF-LHIMUNV E3RF25BD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92440-BM,E3RF-LHIMUNV E3RF25BD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92440-NBM,E3RF-LHIMUNV E3RF25BD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92440-WM,E3RF-LHIMUNV E3RF25BD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92740-BM,E3RF-LHIMUNV E3RF25BD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92740-NBM,E3RF-LHIMUNV E3RF25BD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92740-WM,E3RF-LHIMUNV E3RF25BD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93040-BM,E3RF-LHIMUNV E3RF25BD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93040-NBM,E3RF-LHIMUNV E3RF25BD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93040-WM,E3RF-LHIMUNV E3RF25BD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93540-BM,E3RF-LHIMUNV E3RF25BD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93540-NBM,E3RF-LHIMUNV E3RF25BD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93540-WM,E3RF-LHIMUNV E3RF25BD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD9WD40-BM,E3RF-LHIMUNV E3RF25BD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD9WD40-NBM,E3RF-LHIMUNV E3RF25BD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD9WD40-WM,E3RF-LHIMUNV E3RF25BD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF25BD92240-BM,E3RF-LOIMUNV E3RF25BD92240-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF25BD92240-NBM,E3RF-LOIMUNV E3RF25BD92240-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF25BD92240-WM,E3RF-LOIMUNV E3RF25BD92240-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF25BD92440-BM,E3RF-LOIMUNV E3RF25BD92440-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF25BD92440-NBM,E3RF-LOIMUNV E3RF25BD92440-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF25BD92440-WM,E3RF-LOIMUNV E3RF25BD92440-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF25BD92740-BM,E3RF-LOIMUNV E3RF25BD92740-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF25BD92740-NBM,E3RF-LOIMUNV E3RF25BD92740-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF25BD92740-WM,E3RF-LOIMUNV E3RF25BD92740-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF25BD93040-BM,E3RF-LOIMUNV E3RF25BD93040-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF25BD93040-NBM,E3RF-LOIMUNV E3RF25BD93040-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF25BD93040-WM,E3RF-LOIMUNV E3RF25BD93040-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF25BD93540-BM,E3RF-LOIMUNV E3RF25BD93540-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF25BD93540-NBM,E3RF-LOIMUNV E3RF25BD93540-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF25BD93540-WM,E3RF-LOIMUNV E3RF25BD93540-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LOIMUNV E3RF25BD9WD40-BM,E3RF-LOIMUNV E3RF25BD9WD40-BM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LOIMUNV E3RF25BD9WD40-NBM,E3RF-LOIMUNV E3RF25BD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LOIMUNV E3RF25BD9WD40-WM,E3RF-LOIMUNV E3RF25BD9WD40-WM,"ELEMENT 3"" ROUND",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92260-BM,E3RF-LHIMUNV E3RF25BD92260-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92260-NBM,E3RF-LHIMUNV E3RF25BD92260-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92260-WM,E3RF-LHIMUNV E3RF25BD92260-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92460-BM,E3RF-LHIMUNV E3RF25BD92460-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92460-NBM,E3RF-LHIMUNV E3RF25BD92460-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92460-WM,E3RF-LHIMUNV E3RF25BD92460-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD92760-BM,E3RF-LHIMUNV E3RF25BD92760-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD92760-NBM,E3RF-LHIMUNV E3RF25BD92760-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD92760-WM,E3RF-LHIMUNV E3RF25BD92760-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93060-BM,E3RF-LHIMUNV E3RF25BD93060-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93060-NBM,E3RF-LHIMUNV E3RF25BD93060-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93060-WM,E3RF-LHIMUNV E3RF25BD93060-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD93560-BM,E3RF-LHIMUNV E3RF25BD93560-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD93560-NBM,E3RF-LHIMUNV E3RF25BD93560-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD93560-WM,E3RF-LHIMUNV E3RF25BD93560-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,1,4,Metal - Visual Comfort & Co. - White Brass
E3RF-LHIMUNV E3RF25BD9WD60-BM,E3RF-LHIMUNV E3RF25BD9WD60-BM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,4,Metal - Visual Comfort & Co. - Black Brass
E3RF-LHIMUNV E3RF25BD9WD60-NBM,E3RF-LHIMUNV E3RF25BD9WD60-NBM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,4,Metal - Visual Comfort & Co. - Natural Brass
E3RF-LHIMUNV E3RF25BD9WD60-WM,E3RF-LHIMUNV E3RF25BD9WD60-WM,"ELEMENT 3"" ROUND",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,1,4,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92218-BM,E3RL-LHIMUNV E3RLBD92218-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92218-NBM,E3RL-LHIMUNV E3RLBD92218-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92218-WM,E3RL-LHIMUNV E3RLBD92218-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92418-BM,E3RL-LHIMUNV E3RLBD92418-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92418-NBM,E3RL-LHIMUNV E3RLBD92418-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92418-WM,E3RL-LHIMUNV E3RLBD92418-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92718-BM,E3RL-LHIMUNV E3RLBD92718-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92718-NBM,E3RL-LHIMUNV E3RLBD92718-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92718-WM,E3RL-LHIMUNV E3RLBD92718-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93018-BM,E3RL-LHIMUNV E3RLBD93018-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93018-NBM,E3RL-LHIMUNV E3RLBD93018-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93018-WM,E3RL-LHIMUNV E3RLBD93018-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93518-BM,E3RL-LHIMUNV E3RLBD93518-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93518-NBM,E3RL-LHIMUNV E3RLBD93518-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93518-WM,E3RL-LHIMUNV E3RLBD93518-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD9WD18-BM,E3RL-LHIMUNV E3RLBD9WD18-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD9WD18-NBM,E3RL-LHIMUNV E3RLBD9WD18-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD9WD18-WM,E3RL-LHIMUNV E3RLBD9WD18-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92225-BM,E3RL-LHIMUNV E3RLBD92225-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92225-NBM,E3RL-LHIMUNV E3RLBD92225-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92225-WM,E3RL-LHIMUNV E3RLBD92225-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92425-BM,E3RL-LHIMUNV E3RLBD92425-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92425-NBM,E3RL-LHIMUNV E3RLBD92425-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92425-WM,E3RL-LHIMUNV E3RLBD92425-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92725-BM,E3RL-LHIMUNV E3RLBD92725-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92725-NBM,E3RL-LHIMUNV E3RLBD92725-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92725-WM,E3RL-LHIMUNV E3RLBD92725-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93025-BM,E3RL-LHIMUNV E3RLBD93025-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93025-NBM,E3RL-LHIMUNV E3RLBD93025-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93025-WM,E3RL-LHIMUNV E3RLBD93025-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93525-BM,E3RL-LHIMUNV E3RLBD93525-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93525-NBM,E3RL-LHIMUNV E3RLBD93525-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93525-WM,E3RL-LHIMUNV E3RLBD93525-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD9WD25-BM,E3RL-LHIMUNV E3RLBD9WD25-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD9WD25-NBM,E3RL-LHIMUNV E3RLBD9WD25-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD9WD25-WM,E3RL-LHIMUNV E3RLBD9WD25-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92240-BM,E3RL-LHIMUNV E3RLBD92240-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92240-NBM,E3RL-LHIMUNV E3RLBD92240-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92240-WM,E3RL-LHIMUNV E3RLBD92240-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92440-BM,E3RL-LHIMUNV E3RLBD92440-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92440-NBM,E3RL-LHIMUNV E3RLBD92440-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92440-WM,E3RL-LHIMUNV E3RLBD92440-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92740-BM,E3RL-LHIMUNV E3RLBD92740-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92740-NBM,E3RL-LHIMUNV E3RLBD92740-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92740-WM,E3RL-LHIMUNV E3RLBD92740-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93040-BM,E3RL-LHIMUNV E3RLBD93040-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93040-NBM,E3RL-LHIMUNV E3RLBD93040-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93040-WM,E3RL-LHIMUNV E3RLBD93040-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93540-BM,E3RL-LHIMUNV E3RLBD93540-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93540-NBM,E3RL-LHIMUNV E3RLBD93540-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93540-WM,E3RL-LHIMUNV E3RLBD93540-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD9WD40-BM,E3RL-LHIMUNV E3RLBD9WD40-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD9WD40-NBM,E3RL-LHIMUNV E3RLBD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD9WD40-WM,E3RL-LHIMUNV E3RLBD9WD40-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LOIMUNV E3RLBD92240-BM,E3RL-LOIMUNV E3RLBD92240-BM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LOIMUNV E3RLBD92240-NBM,E3RL-LOIMUNV E3RLBD92240-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LOIMUNV E3RLBD92240-WM,E3RL-LOIMUNV E3RLBD92240-WM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LOIMUNV E3RLBD92440-BM,E3RL-LOIMUNV E3RLBD92440-BM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LOIMUNV E3RLBD92440-NBM,E3RL-LOIMUNV E3RLBD92440-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LOIMUNV E3RLBD92440-WM,E3RL-LOIMUNV E3RLBD92440-WM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LOIMUNV E3RLBD92740-BM,E3RL-LOIMUNV E3RLBD92740-BM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LOIMUNV E3RLBD92740-NBM,E3RL-LOIMUNV E3RLBD92740-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LOIMUNV E3RLBD92740-WM,E3RL-LOIMUNV E3RLBD92740-WM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LOIMUNV E3RLBD93040-BM,E3RL-LOIMUNV E3RLBD93040-BM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LOIMUNV E3RLBD93040-NBM,E3RL-LOIMUNV E3RLBD93040-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LOIMUNV E3RLBD93040-WM,E3RL-LOIMUNV E3RLBD93040-WM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LOIMUNV E3RLBD93540-BM,E3RL-LOIMUNV E3RLBD93540-BM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LOIMUNV E3RLBD93540-NBM,E3RL-LOIMUNV E3RLBD93540-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LOIMUNV E3RLBD93540-WM,E3RL-LOIMUNV E3RLBD93540-WM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LOIMUNV E3RLBD9WD40-BM,E3RL-LOIMUNV E3RLBD9WD40-BM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LOIMUNV E3RLBD9WD40-NBM,E3RL-LOIMUNV E3RLBD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LOIMUNV E3RLBD9WD40-WM,E3RL-LOIMUNV E3RLBD9WD40-WM,"ELEMENT 3"" ROUND",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92260-BM,E3RL-LHIMUNV E3RLBD92260-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92260-NBM,E3RL-LHIMUNV E3RLBD92260-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92260-WM,E3RL-LHIMUNV E3RLBD92260-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92460-BM,E3RL-LHIMUNV E3RLBD92460-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92460-NBM,E3RL-LHIMUNV E3RLBD92460-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92460-WM,E3RL-LHIMUNV E3RLBD92460-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD92760-BM,E3RL-LHIMUNV E3RLBD92760-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD92760-NBM,E3RL-LHIMUNV E3RLBD92760-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD92760-WM,E3RL-LHIMUNV E3RLBD92760-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93060-BM,E3RL-LHIMUNV E3RLBD93060-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93060-NBM,E3RL-LHIMUNV E3RLBD93060-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93060-WM,E3RL-LHIMUNV E3RLBD93060-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD93560-BM,E3RL-LHIMUNV E3RLBD93560-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD93560-NBM,E3RL-LHIMUNV E3RLBD93560-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD93560-WM,E3RL-LHIMUNV E3RLBD93560-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RL-LHIMUNV E3RLBD9WD60-BM,E3RL-LHIMUNV E3RLBD9WD60-BM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RL-LHIMUNV E3RLBD9WD60-NBM,E3RL-LHIMUNV E3RLBD9WD60-NBM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RL-LHIMUNV E3RLBD9WD60-WM,E3RL-LHIMUNV E3RLBD9WD60-WM,"ELEMENT 3"" ROUND",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92218-BM,E3RWC-LHIMUNV E3RLBD92218-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92218-NBM,E3RWC-LHIMUNV E3RLBD92218-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92218-WM,E3RWC-LHIMUNV E3RLBD92218-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92418-BM,E3RWC-LHIMUNV E3RLBD92418-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92418-NBM,E3RWC-LHIMUNV E3RLBD92418-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92418-WM,E3RWC-LHIMUNV E3RLBD92418-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92718-BM,E3RWC-LHIMUNV E3RLBD92718-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92718-NBM,E3RWC-LHIMUNV E3RLBD92718-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92718-WM,E3RWC-LHIMUNV E3RLBD92718-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93018-BM,E3RWC-LHIMUNV E3RLBD93018-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93018-NBM,E3RWC-LHIMUNV E3RLBD93018-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93018-WM,E3RWC-LHIMUNV E3RLBD93018-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93018-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93518-BM,E3RWC-LHIMUNV E3RLBD93518-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93518-NBM,E3RWC-LHIMUNV E3RLBD93518-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93518-WM,E3RWC-LHIMUNV E3RLBD93518-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD9WD18-BM,E3RWC-LHIMUNV E3RLBD9WD18-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD9WD18-NBM,E3RWC-LHIMUNV E3RLBD9WD18-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD9WD18-WM,E3RWC-LHIMUNV E3RLBD9WD18-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD18-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92225-BM,E3RWC-LHIMUNV E3RLBD92225-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92225-NBM,E3RWC-LHIMUNV E3RLBD92225-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92225-WM,E3RWC-LHIMUNV E3RLBD92225-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92425-BM,E3RWC-LHIMUNV E3RLBD92425-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92425-NBM,E3RWC-LHIMUNV E3RLBD92425-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92425-WM,E3RWC-LHIMUNV E3RLBD92425-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92725-BM,E3RWC-LHIMUNV E3RLBD92725-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92725-NBM,E3RWC-LHIMUNV E3RLBD92725-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92725-WM,E3RWC-LHIMUNV E3RLBD92725-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93025-BM,E3RWC-LHIMUNV E3RLBD93025-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93025-NBM,E3RWC-LHIMUNV E3RLBD93025-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93025-WM,E3RWC-LHIMUNV E3RLBD93025-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93025-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93525-BM,E3RWC-LHIMUNV E3RLBD93525-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93525-NBM,E3RWC-LHIMUNV E3RLBD93525-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93525-WM,E3RWC-LHIMUNV E3RLBD93525-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD9WD25-BM,E3RWC-LHIMUNV E3RLBD9WD25-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD9WD25-NBM,E3RWC-LHIMUNV E3RLBD9WD25-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD9WD25-WM,E3RWC-LHIMUNV E3RLBD9WD25-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD25-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92240-BM,E3RWC-LHIMUNV E3RLBD92240-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92240-NBM,E3RWC-LHIMUNV E3RLBD92240-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92240-WM,E3RWC-LHIMUNV E3RLBD92240-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92440-BM,E3RWC-LHIMUNV E3RLBD92440-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92440-NBM,E3RWC-LHIMUNV E3RLBD92440-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92440-WM,E3RWC-LHIMUNV E3RLBD92440-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92740-BM,E3RWC-LHIMUNV E3RLBD92740-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92740-NBM,E3RWC-LHIMUNV E3RLBD92740-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92740-WM,E3RWC-LHIMUNV E3RLBD92740-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93040-BM,E3RWC-LHIMUNV E3RLBD93040-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93040-NBM,E3RWC-LHIMUNV E3RLBD93040-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93040-WM,E3RWC-LHIMUNV E3RLBD93040-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93540-BM,E3RWC-LHIMUNV E3RLBD93540-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93540-NBM,E3RWC-LHIMUNV E3RLBD93540-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93540-WM,E3RWC-LHIMUNV E3RLBD93540-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD9WD40-BM,E3RWC-LHIMUNV E3RLBD9WD40-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD9WD40-NBM,E3RWC-LHIMUNV E3RLBD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD9WD40-WM,E3RWC-LHIMUNV E3RLBD9WD40-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD40-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LOIMUNV E3RLBD92240-BM,E3RWC-LOIMUNV E3RLBD92240-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LOIMUNV E3RLBD92240-NBM,E3RWC-LOIMUNV E3RLBD92240-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LOIMUNV E3RLBD92240-WM,E3RWC-LOIMUNV E3RLBD92240-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LOIMUNV E3RLBD92440-BM,E3RWC-LOIMUNV E3RLBD92440-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LOIMUNV E3RLBD92440-NBM,E3RWC-LOIMUNV E3RLBD92440-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LOIMUNV E3RLBD92440-WM,E3RWC-LOIMUNV E3RLBD92440-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LOIMUNV E3RLBD92740-BM,E3RWC-LOIMUNV E3RLBD92740-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LOIMUNV E3RLBD92740-NBM,E3RWC-LOIMUNV E3RLBD92740-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LOIMUNV E3RLBD92740-WM,E3RWC-LOIMUNV E3RLBD92740-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LOIMUNV E3RLBD93040-BM,E3RWC-LOIMUNV E3RLBD93040-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LOIMUNV E3RLBD93040-NBM,E3RWC-LOIMUNV E3RLBD93040-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LOIMUNV E3RLBD93040-WM,E3RWC-LOIMUNV E3RLBD93040-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,E3RF-LOIMUNV E3RFBD93040-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LOIMUNV E3RLBD93540-BM,E3RWC-LOIMUNV E3RLBD93540-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LOIMUNV E3RLBD93540-NBM,E3RWC-LOIMUNV E3RLBD93540-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LOIMUNV E3RLBD93540-WM,E3RWC-LOIMUNV E3RLBD93540-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LOIMUNV E3RLBD9WD40-BM,E3RWC-LOIMUNV E3RLBD9WD40-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LOIMUNV E3RLBD9WD40-NBM,E3RWC-LOIMUNV E3RLBD9WD40-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LOIMUNV E3RLBD9WD40-WM,E3RWC-LOIMUNV E3RLBD9WD40-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92260-BM,E3RWC-LHIMUNV E3RLBD92260-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92260-NBM,E3RWC-LHIMUNV E3RLBD92260-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92260-WM,E3RWC-LHIMUNV E3RLBD92260-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92460-BM,E3RWC-LHIMUNV E3RLBD92460-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92460-NBM,E3RWC-LHIMUNV E3RLBD92460-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92460-WM,E3RWC-LHIMUNV E3RLBD92460-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD92760-BM,E3RWC-LHIMUNV E3RLBD92760-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD92760-NBM,E3RWC-LHIMUNV E3RLBD92760-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD92760-WM,E3RWC-LHIMUNV E3RLBD92760-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93060-BM,E3RWC-LHIMUNV E3RLBD93060-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93060-NBM,E3RWC-LHIMUNV E3RLBD93060-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93060-WM,E3RWC-LHIMUNV E3RLBD93060-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD93060-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD93560-BM,E3RWC-LHIMUNV E3RLBD93560-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD93560-NBM,E3RWC-LHIMUNV E3RLBD93560-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD93560-WM,E3RWC-LHIMUNV E3RLBD93560-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,2,1,Metal - Visual Comfort & Co. - White Brass
E3RWC-LHIMUNV E3RLBD9WD60-BM,E3RWC-LHIMUNV E3RLBD9WD60-BM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,2,1,Metal - Visual Comfort & Co. - Black Brass
E3RWC-LHIMUNV E3RLBD9WD60-NBM,E3RWC-LHIMUNV E3RLBD9WD60-NBM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,2,1,Metal - Visual Comfort & Co. - Natural Brass
E3RWC-LHIMUNV E3RLBD9WD60-WM,E3RWC-LHIMUNV E3RLBD9WD60-WM,"ELEMENT 3"" ROUND",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" ROUND MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3RF-LHIMUNV E3RFBD9WD60-WM.ies,2,1,Metal - Visual Comfort & Co. - White Brass
