,Model##other##,Product (Housing)##other##,Ceiling Appearance (Housing)##other##,Output (Housing)##other##,Driver (Housing)##other##,Product (Trim)##other##,Ceiling Appearance (Trim)##other##,Style (Trim)##other##,Function (Trim)##other##,LED (Trim)##other##,Beam Spread (Trim)##other##,Finish (Trim)##other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Wattage Comments##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Photometric Web File##OTHER##,Constraints##other##,Constraints Ceiling##other##,Finish##other##
E3SF-LHIMUNV E3SFBD92218-BM,E3SF-LHIMUNV E3SFBD92218-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92218-NBM,E3SF-LHIMUNV E3SFBD92218-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92218-WM,E3SF-LHIMUNV E3SFBD92218-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92418-BM,E3SF-LHIMUNV E3SFBD92418-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92418-NBM,E3SF-LHIMUNV E3SFBD92418-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92418-WM,E3SF-LHIMUNV E3SFBD92418-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92718-BM,E3SF-LHIMUNV E3SFBD92718-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92718-NBM,E3SF-LHIMUNV E3SFBD92718-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92718-WM,E3SF-LHIMUNV E3SFBD92718-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93018-BM,E3SF-LHIMUNV E3SFBD93018-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93018-NBM,E3SF-LHIMUNV E3SFBD93018-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93018-WM,E3SF-LHIMUNV E3SFBD93018-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93518-BM,E3SF-LHIMUNV E3SFBD93518-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93518-NBM,E3SF-LHIMUNV E3SFBD93518-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93518-WM,E3SF-LHIMUNV E3SFBD93518-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD9WD18-BM,E3SF-LHIMUNV E3SFBD9WD18-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD9WD18-NBM,E3SF-LHIMUNV E3SFBD9WD18-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD9WD18-WM,E3SF-LHIMUNV E3SFBD9WD18-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92225-BM,E3SF-LHIMUNV E3SFBD92225-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92225-NBM,E3SF-LHIMUNV E3SFBD92225-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92225-WM,E3SF-LHIMUNV E3SFBD92225-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92425-BM,E3SF-LHIMUNV E3SFBD92425-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92425-NBM,E3SF-LHIMUNV E3SFBD92425-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92425-WM,E3SF-LHIMUNV E3SFBD92425-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92725-BM,E3SF-LHIMUNV E3SFBD92725-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92725-NBM,E3SF-LHIMUNV E3SFBD92725-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92725-WM,E3SF-LHIMUNV E3SFBD92725-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93025-BM,E3SF-LHIMUNV E3SFBD93025-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93025-NBM,E3SF-LHIMUNV E3SFBD93025-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93025-WM,E3SF-LHIMUNV E3SFBD93025-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93525-BM,E3SF-LHIMUNV E3SFBD93525-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93525-NBM,E3SF-LHIMUNV E3SFBD93525-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93525-WM,E3SF-LHIMUNV E3SFBD93525-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD9WD25-BM,E3SF-LHIMUNV E3SFBD9WD25-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD9WD25-NBM,E3SF-LHIMUNV E3SFBD9WD25-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD9WD25-WM,E3SF-LHIMUNV E3SFBD9WD25-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92240-BM,E3SF-LHIMUNV E3SFBD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92240-NBM,E3SF-LHIMUNV E3SFBD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92240-WM,E3SF-LHIMUNV E3SFBD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92440-BM,E3SF-LHIMUNV E3SFBD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92440-NBM,E3SF-LHIMUNV E3SFBD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92440-WM,E3SF-LHIMUNV E3SFBD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92740-BM,E3SF-LHIMUNV E3SFBD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92740-NBM,E3SF-LHIMUNV E3SFBD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92740-WM,E3SF-LHIMUNV E3SFBD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93040-BM,E3SF-LHIMUNV E3SFBD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93040-NBM,E3SF-LHIMUNV E3SFBD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93040-WM,E3SF-LHIMUNV E3SFBD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93540-BM,E3SF-LHIMUNV E3SFBD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93540-NBM,E3SF-LHIMUNV E3SFBD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93540-WM,E3SF-LHIMUNV E3SFBD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD9WD40-BM,E3SF-LHIMUNV E3SFBD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD9WD40-NBM,E3SF-LHIMUNV E3SFBD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD9WD40-WM,E3SF-LHIMUNV E3SFBD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SFBD92240-BM,E3SF-LOIMUNV E3SFBD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SFBD92240-NBM,E3SF-LOIMUNV E3SFBD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SFBD92240-WM,E3SF-LOIMUNV E3SFBD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SFBD92440-BM,E3SF-LOIMUNV E3SFBD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SFBD92440-NBM,E3SF-LOIMUNV E3SFBD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SFBD92440-WM,E3SF-LOIMUNV E3SFBD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SFBD92740-BM,E3SF-LOIMUNV E3SFBD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SFBD92740-NBM,E3SF-LOIMUNV E3SFBD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SFBD92740-WM,E3SF-LOIMUNV E3SFBD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SFBD93040-BM,E3SF-LOIMUNV E3SFBD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SFBD93040-NBM,E3SF-LOIMUNV E3SFBD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SFBD93040-WM,E3SF-LOIMUNV E3SFBD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SFBD93540-BM,E3SF-LOIMUNV E3SFBD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SFBD93540-NBM,E3SF-LOIMUNV E3SFBD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SFBD93540-WM,E3SF-LOIMUNV E3SFBD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SFBD9WD40-BM,E3SF-LOIMUNV E3SFBD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SFBD9WD40-NBM,E3SF-LOIMUNV E3SFBD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SFBD9WD40-WM,E3SF-LOIMUNV E3SFBD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92260-BM,E3SF-LHIMUNV E3SFBD92260-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92260-NBM,E3SF-LHIMUNV E3SFBD92260-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92260-WM,E3SF-LHIMUNV E3SFBD92260-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92460-BM,E3SF-LHIMUNV E3SFBD92460-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92460-NBM,E3SF-LHIMUNV E3SFBD92460-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92460-WM,E3SF-LHIMUNV E3SFBD92460-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD92760-BM,E3SF-LHIMUNV E3SFBD92760-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD92760-NBM,E3SF-LHIMUNV E3SFBD92760-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD92760-WM,E3SF-LHIMUNV E3SFBD92760-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93060-BM,E3SF-LHIMUNV E3SFBD93060-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93060-NBM,E3SF-LHIMUNV E3SFBD93060-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93060-WM,E3SF-LHIMUNV E3SFBD93060-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD93560-BM,E3SF-LHIMUNV E3SFBD93560-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD93560-NBM,E3SF-LHIMUNV E3SFBD93560-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD93560-WM,E3SF-LHIMUNV E3SFBD93560-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SFBD9WD60-BM,E3SF-LHIMUNV E3SFBD9WD60-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,1,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SFBD9WD60-NBM,E3SF-LHIMUNV E3SFBD9WD60-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,1,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SFBD9WD60-WM,E3SF-LHIMUNV E3SFBD9WD60-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED UP TO 1"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,1,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92218-BM,E3SF-LHIMUNV E3SF15BD92218-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92218-NBM,E3SF-LHIMUNV E3SF15BD92218-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92218-WM,E3SF-LHIMUNV E3SF15BD92218-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92418-BM,E3SF-LHIMUNV E3SF15BD92418-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92418-NBM,E3SF-LHIMUNV E3SF15BD92418-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92418-WM,E3SF-LHIMUNV E3SF15BD92418-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92718-BM,E3SF-LHIMUNV E3SF15BD92718-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92718-NBM,E3SF-LHIMUNV E3SF15BD92718-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92718-WM,E3SF-LHIMUNV E3SF15BD92718-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93018-BM,E3SF-LHIMUNV E3SF15BD93018-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93018-NBM,E3SF-LHIMUNV E3SF15BD93018-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93018-WM,E3SF-LHIMUNV E3SF15BD93018-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93518-BM,E3SF-LHIMUNV E3SF15BD93518-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93518-NBM,E3SF-LHIMUNV E3SF15BD93518-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93518-WM,E3SF-LHIMUNV E3SF15BD93518-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD9WD18-BM,E3SF-LHIMUNV E3SF15BD9WD18-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD9WD18-NBM,E3SF-LHIMUNV E3SF15BD9WD18-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD9WD18-WM,E3SF-LHIMUNV E3SF15BD9WD18-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92225-BM,E3SF-LHIMUNV E3SF15BD92225-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92225-NBM,E3SF-LHIMUNV E3SF15BD92225-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92225-WM,E3SF-LHIMUNV E3SF15BD92225-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92425-BM,E3SF-LHIMUNV E3SF15BD92425-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92425-NBM,E3SF-LHIMUNV E3SF15BD92425-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92425-WM,E3SF-LHIMUNV E3SF15BD92425-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92725-BM,E3SF-LHIMUNV E3SF15BD92725-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92725-NBM,E3SF-LHIMUNV E3SF15BD92725-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92725-WM,E3SF-LHIMUNV E3SF15BD92725-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93025-BM,E3SF-LHIMUNV E3SF15BD93025-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93025-NBM,E3SF-LHIMUNV E3SF15BD93025-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93025-WM,E3SF-LHIMUNV E3SF15BD93025-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93525-BM,E3SF-LHIMUNV E3SF15BD93525-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93525-NBM,E3SF-LHIMUNV E3SF15BD93525-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93525-WM,E3SF-LHIMUNV E3SF15BD93525-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD9WD25-BM,E3SF-LHIMUNV E3SF15BD9WD25-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD9WD25-NBM,E3SF-LHIMUNV E3SF15BD9WD25-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD9WD25-WM,E3SF-LHIMUNV E3SF15BD9WD25-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92240-BM,E3SF-LHIMUNV E3SF15BD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92240-NBM,E3SF-LHIMUNV E3SF15BD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92240-WM,E3SF-LHIMUNV E3SF15BD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92440-BM,E3SF-LHIMUNV E3SF15BD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92440-NBM,E3SF-LHIMUNV E3SF15BD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92440-WM,E3SF-LHIMUNV E3SF15BD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92740-BM,E3SF-LHIMUNV E3SF15BD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92740-NBM,E3SF-LHIMUNV E3SF15BD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92740-WM,E3SF-LHIMUNV E3SF15BD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93040-BM,E3SF-LHIMUNV E3SF15BD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93040-NBM,E3SF-LHIMUNV E3SF15BD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93040-WM,E3SF-LHIMUNV E3SF15BD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93540-BM,E3SF-LHIMUNV E3SF15BD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93540-NBM,E3SF-LHIMUNV E3SF15BD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93540-WM,E3SF-LHIMUNV E3SF15BD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD9WD40-BM,E3SF-LHIMUNV E3SF15BD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD9WD40-NBM,E3SF-LHIMUNV E3SF15BD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD9WD40-WM,E3SF-LHIMUNV E3SF15BD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF15BD92240-BM,E3SF-LOIMUNV E3SF15BD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF15BD92240-NBM,E3SF-LOIMUNV E3SF15BD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF15BD92240-WM,E3SF-LOIMUNV E3SF15BD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF15BD92440-BM,E3SF-LOIMUNV E3SF15BD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF15BD92440-NBM,E3SF-LOIMUNV E3SF15BD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF15BD92440-WM,E3SF-LOIMUNV E3SF15BD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF15BD92740-BM,E3SF-LOIMUNV E3SF15BD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF15BD92740-NBM,E3SF-LOIMUNV E3SF15BD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF15BD92740-WM,E3SF-LOIMUNV E3SF15BD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF15BD93040-BM,E3SF-LOIMUNV E3SF15BD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF15BD93040-NBM,E3SF-LOIMUNV E3SF15BD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF15BD93040-WM,E3SF-LOIMUNV E3SF15BD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF15BD93540-BM,E3SF-LOIMUNV E3SF15BD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF15BD93540-NBM,E3SF-LOIMUNV E3SF15BD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF15BD93540-WM,E3SF-LOIMUNV E3SF15BD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF15BD9WD40-BM,E3SF-LOIMUNV E3SF15BD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF15BD9WD40-NBM,E3SF-LOIMUNV E3SF15BD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF15BD9WD40-WM,E3SF-LOIMUNV E3SF15BD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92260-BM,E3SF-LHIMUNV E3SF15BD92260-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92260-NBM,E3SF-LHIMUNV E3SF15BD92260-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92260-WM,E3SF-LHIMUNV E3SF15BD92260-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92460-BM,E3SF-LHIMUNV E3SF15BD92460-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92460-NBM,E3SF-LHIMUNV E3SF15BD92460-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92460-WM,E3SF-LHIMUNV E3SF15BD92460-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD92760-BM,E3SF-LHIMUNV E3SF15BD92760-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD92760-NBM,E3SF-LHIMUNV E3SF15BD92760-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD92760-WM,E3SF-LHIMUNV E3SF15BD92760-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93060-BM,E3SF-LHIMUNV E3SF15BD93060-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93060-NBM,E3SF-LHIMUNV E3SF15BD93060-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93060-WM,E3SF-LHIMUNV E3SF15BD93060-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD93560-BM,E3SF-LHIMUNV E3SF15BD93560-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD93560-NBM,E3SF-LHIMUNV E3SF15BD93560-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD93560-WM,E3SF-LHIMUNV E3SF15BD93560-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF15BD9WD60-BM,E3SF-LHIMUNV E3SF15BD9WD60-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,2,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF15BD9WD60-NBM,E3SF-LHIMUNV E3SF15BD9WD60-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,2,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF15BD9WD60-WM,E3SF-LHIMUNV E3SF15BD9WD60-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.1""-1.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,2,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92218-BM,E3SF-LHIMUNV E3SF20BD92218-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92218-NBM,E3SF-LHIMUNV E3SF20BD92218-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92218-WM,E3SF-LHIMUNV E3SF20BD92218-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92418-BM,E3SF-LHIMUNV E3SF20BD92418-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92418-NBM,E3SF-LHIMUNV E3SF20BD92418-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92418-WM,E3SF-LHIMUNV E3SF20BD92418-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92718-BM,E3SF-LHIMUNV E3SF20BD92718-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92718-NBM,E3SF-LHIMUNV E3SF20BD92718-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92718-WM,E3SF-LHIMUNV E3SF20BD92718-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93018-BM,E3SF-LHIMUNV E3SF20BD93018-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93018-NBM,E3SF-LHIMUNV E3SF20BD93018-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93018-WM,E3SF-LHIMUNV E3SF20BD93018-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93518-BM,E3SF-LHIMUNV E3SF20BD93518-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93518-NBM,E3SF-LHIMUNV E3SF20BD93518-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93518-WM,E3SF-LHIMUNV E3SF20BD93518-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD9WD18-BM,E3SF-LHIMUNV E3SF20BD9WD18-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD9WD18-NBM,E3SF-LHIMUNV E3SF20BD9WD18-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD9WD18-WM,E3SF-LHIMUNV E3SF20BD9WD18-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92225-BM,E3SF-LHIMUNV E3SF20BD92225-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92225-NBM,E3SF-LHIMUNV E3SF20BD92225-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92225-WM,E3SF-LHIMUNV E3SF20BD92225-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92425-BM,E3SF-LHIMUNV E3SF20BD92425-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92425-NBM,E3SF-LHIMUNV E3SF20BD92425-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92425-WM,E3SF-LHIMUNV E3SF20BD92425-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92725-BM,E3SF-LHIMUNV E3SF20BD92725-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92725-NBM,E3SF-LHIMUNV E3SF20BD92725-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92725-WM,E3SF-LHIMUNV E3SF20BD92725-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93025-BM,E3SF-LHIMUNV E3SF20BD93025-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93025-NBM,E3SF-LHIMUNV E3SF20BD93025-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93025-WM,E3SF-LHIMUNV E3SF20BD93025-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93525-BM,E3SF-LHIMUNV E3SF20BD93525-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93525-NBM,E3SF-LHIMUNV E3SF20BD93525-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93525-WM,E3SF-LHIMUNV E3SF20BD93525-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD9WD25-BM,E3SF-LHIMUNV E3SF20BD9WD25-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD9WD25-NBM,E3SF-LHIMUNV E3SF20BD9WD25-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD9WD25-WM,E3SF-LHIMUNV E3SF20BD9WD25-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92240-BM,E3SF-LHIMUNV E3SF20BD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92240-NBM,E3SF-LHIMUNV E3SF20BD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92240-WM,E3SF-LHIMUNV E3SF20BD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92440-BM,E3SF-LHIMUNV E3SF20BD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92440-NBM,E3SF-LHIMUNV E3SF20BD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92440-WM,E3SF-LHIMUNV E3SF20BD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92740-BM,E3SF-LHIMUNV E3SF20BD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92740-NBM,E3SF-LHIMUNV E3SF20BD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92740-WM,E3SF-LHIMUNV E3SF20BD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93040-BM,E3SF-LHIMUNV E3SF20BD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93040-NBM,E3SF-LHIMUNV E3SF20BD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93040-WM,E3SF-LHIMUNV E3SF20BD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93540-BM,E3SF-LHIMUNV E3SF20BD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93540-NBM,E3SF-LHIMUNV E3SF20BD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93540-WM,E3SF-LHIMUNV E3SF20BD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD9WD40-BM,E3SF-LHIMUNV E3SF20BD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD9WD40-NBM,E3SF-LHIMUNV E3SF20BD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD9WD40-WM,E3SF-LHIMUNV E3SF20BD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF20BD92240-BM,E3SF-LOIMUNV E3SF20BD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF20BD92240-NBM,E3SF-LOIMUNV E3SF20BD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF20BD92240-WM,E3SF-LOIMUNV E3SF20BD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF20BD92440-BM,E3SF-LOIMUNV E3SF20BD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF20BD92440-NBM,E3SF-LOIMUNV E3SF20BD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF20BD92440-WM,E3SF-LOIMUNV E3SF20BD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF20BD92740-BM,E3SF-LOIMUNV E3SF20BD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF20BD92740-NBM,E3SF-LOIMUNV E3SF20BD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF20BD92740-WM,E3SF-LOIMUNV E3SF20BD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF20BD93040-BM,E3SF-LOIMUNV E3SF20BD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF20BD93040-NBM,E3SF-LOIMUNV E3SF20BD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF20BD93040-WM,E3SF-LOIMUNV E3SF20BD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF20BD93540-BM,E3SF-LOIMUNV E3SF20BD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF20BD93540-NBM,E3SF-LOIMUNV E3SF20BD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF20BD93540-WM,E3SF-LOIMUNV E3SF20BD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF20BD9WD40-BM,E3SF-LOIMUNV E3SF20BD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF20BD9WD40-NBM,E3SF-LOIMUNV E3SF20BD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF20BD9WD40-WM,E3SF-LOIMUNV E3SF20BD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92260-BM,E3SF-LHIMUNV E3SF20BD92260-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92260-NBM,E3SF-LHIMUNV E3SF20BD92260-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92260-WM,E3SF-LHIMUNV E3SF20BD92260-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92460-BM,E3SF-LHIMUNV E3SF20BD92460-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92460-NBM,E3SF-LHIMUNV E3SF20BD92460-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92460-WM,E3SF-LHIMUNV E3SF20BD92460-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD92760-BM,E3SF-LHIMUNV E3SF20BD92760-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD92760-NBM,E3SF-LHIMUNV E3SF20BD92760-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD92760-WM,E3SF-LHIMUNV E3SF20BD92760-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93060-BM,E3SF-LHIMUNV E3SF20BD93060-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93060-NBM,E3SF-LHIMUNV E3SF20BD93060-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93060-WM,E3SF-LHIMUNV E3SF20BD93060-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD93560-BM,E3SF-LHIMUNV E3SF20BD93560-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD93560-NBM,E3SF-LHIMUNV E3SF20BD93560-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD93560-WM,E3SF-LHIMUNV E3SF20BD93560-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF20BD9WD60-BM,E3SF-LHIMUNV E3SF20BD9WD60-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,3,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF20BD9WD60-NBM,E3SF-LHIMUNV E3SF20BD9WD60-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,3,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF20BD9WD60-WM,E3SF-LHIMUNV E3SF20BD9WD60-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 1.6""-2.0"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,3,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92218-BM,E3SF-LHIMUNV E3SF25BD92218-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92218-NBM,E3SF-LHIMUNV E3SF25BD92218-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92218-WM,E3SF-LHIMUNV E3SF25BD92218-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92418-BM,E3SF-LHIMUNV E3SF25BD92418-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92418-NBM,E3SF-LHIMUNV E3SF25BD92418-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92418-WM,E3SF-LHIMUNV E3SF25BD92418-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92718-BM,E3SF-LHIMUNV E3SF25BD92718-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92718-NBM,E3SF-LHIMUNV E3SF25BD92718-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92718-WM,E3SF-LHIMUNV E3SF25BD92718-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93018-BM,E3SF-LHIMUNV E3SF25BD93018-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93018-NBM,E3SF-LHIMUNV E3SF25BD93018-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93018-WM,E3SF-LHIMUNV E3SF25BD93018-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93518-BM,E3SF-LHIMUNV E3SF25BD93518-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93518-NBM,E3SF-LHIMUNV E3SF25BD93518-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93518-WM,E3SF-LHIMUNV E3SF25BD93518-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD9WD18-BM,E3SF-LHIMUNV E3SF25BD9WD18-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD9WD18-NBM,E3SF-LHIMUNV E3SF25BD9WD18-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD9WD18-WM,E3SF-LHIMUNV E3SF25BD9WD18-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92225-BM,E3SF-LHIMUNV E3SF25BD92225-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92225-NBM,E3SF-LHIMUNV E3SF25BD92225-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92225-WM,E3SF-LHIMUNV E3SF25BD92225-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92425-BM,E3SF-LHIMUNV E3SF25BD92425-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92425-NBM,E3SF-LHIMUNV E3SF25BD92425-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92425-WM,E3SF-LHIMUNV E3SF25BD92425-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92725-BM,E3SF-LHIMUNV E3SF25BD92725-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92725-NBM,E3SF-LHIMUNV E3SF25BD92725-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92725-WM,E3SF-LHIMUNV E3SF25BD92725-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93025-BM,E3SF-LHIMUNV E3SF25BD93025-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93025-NBM,E3SF-LHIMUNV E3SF25BD93025-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93025-WM,E3SF-LHIMUNV E3SF25BD93025-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93525-BM,E3SF-LHIMUNV E3SF25BD93525-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93525-NBM,E3SF-LHIMUNV E3SF25BD93525-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93525-WM,E3SF-LHIMUNV E3SF25BD93525-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD9WD25-BM,E3SF-LHIMUNV E3SF25BD9WD25-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD9WD25-NBM,E3SF-LHIMUNV E3SF25BD9WD25-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD9WD25-WM,E3SF-LHIMUNV E3SF25BD9WD25-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92240-BM,E3SF-LHIMUNV E3SF25BD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92240-NBM,E3SF-LHIMUNV E3SF25BD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92240-WM,E3SF-LHIMUNV E3SF25BD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92440-BM,E3SF-LHIMUNV E3SF25BD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92440-NBM,E3SF-LHIMUNV E3SF25BD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92440-WM,E3SF-LHIMUNV E3SF25BD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92740-BM,E3SF-LHIMUNV E3SF25BD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92740-NBM,E3SF-LHIMUNV E3SF25BD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92740-WM,E3SF-LHIMUNV E3SF25BD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93040-BM,E3SF-LHIMUNV E3SF25BD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93040-NBM,E3SF-LHIMUNV E3SF25BD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93040-WM,E3SF-LHIMUNV E3SF25BD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93540-BM,E3SF-LHIMUNV E3SF25BD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93540-NBM,E3SF-LHIMUNV E3SF25BD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93540-WM,E3SF-LHIMUNV E3SF25BD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD9WD40-BM,E3SF-LHIMUNV E3SF25BD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD9WD40-NBM,E3SF-LHIMUNV E3SF25BD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD9WD40-WM,E3SF-LHIMUNV E3SF25BD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF25BD92240-BM,E3SF-LOIMUNV E3SF25BD92240-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF25BD92240-NBM,E3SF-LOIMUNV E3SF25BD92240-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF25BD92240-WM,E3SF-LOIMUNV E3SF25BD92240-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF25BD92440-BM,E3SF-LOIMUNV E3SF25BD92440-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF25BD92440-NBM,E3SF-LOIMUNV E3SF25BD92440-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF25BD92440-WM,E3SF-LOIMUNV E3SF25BD92440-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF25BD92740-BM,E3SF-LOIMUNV E3SF25BD92740-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF25BD92740-NBM,E3SF-LOIMUNV E3SF25BD92740-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF25BD92740-WM,E3SF-LOIMUNV E3SF25BD92740-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF25BD93040-BM,E3SF-LOIMUNV E3SF25BD93040-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF25BD93040-NBM,E3SF-LOIMUNV E3SF25BD93040-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF25BD93040-WM,E3SF-LOIMUNV E3SF25BD93040-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF25BD93540-BM,E3SF-LOIMUNV E3SF25BD93540-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF25BD93540-NBM,E3SF-LOIMUNV E3SF25BD93540-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF25BD93540-WM,E3SF-LOIMUNV E3SF25BD93540-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LOIMUNV E3SF25BD9WD40-BM,E3SF-LOIMUNV E3SF25BD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LOIMUNV E3SF25BD9WD40-NBM,E3SF-LOIMUNV E3SF25BD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LOIMUNV E3SF25BD9WD40-WM,E3SF-LOIMUNV E3SF25BD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGED,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92260-BM,E3SF-LHIMUNV E3SF25BD92260-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92260-NBM,E3SF-LHIMUNV E3SF25BD92260-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92260-WM,E3SF-LHIMUNV E3SF25BD92260-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92460-BM,E3SF-LHIMUNV E3SF25BD92460-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92460-NBM,E3SF-LHIMUNV E3SF25BD92460-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92460-WM,E3SF-LHIMUNV E3SF25BD92460-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD92760-BM,E3SF-LHIMUNV E3SF25BD92760-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD92760-NBM,E3SF-LHIMUNV E3SF25BD92760-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD92760-WM,E3SF-LHIMUNV E3SF25BD92760-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93060-BM,E3SF-LHIMUNV E3SF25BD93060-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93060-NBM,E3SF-LHIMUNV E3SF25BD93060-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93060-WM,E3SF-LHIMUNV E3SF25BD93060-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD93560-BM,E3SF-LHIMUNV E3SF25BD93560-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD93560-NBM,E3SF-LHIMUNV E3SF25BD93560-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD93560-WM,E3SF-LHIMUNV E3SF25BD93560-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,3,4,Metal - Visual Comfort & Co. - White Brass
E3SF-LHIMUNV E3SF25BD9WD60-BM,E3SF-LHIMUNV E3SF25BD9WD60-BM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,4,Metal - Visual Comfort & Co. - Black Brass
E3SF-LHIMUNV E3SF25BD9WD60-NBM,E3SF-LHIMUNV E3SF25BD9WD60-NBM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,4,Metal - Visual Comfort & Co. - Natural Brass
E3SF-LHIMUNV E3SF25BD9WD60-WM,E3SF-LHIMUNV E3SF25BD9WD60-WM,"ELEMENT 3"" SQUARE",FLANGED,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE","FLANGED 2.1""-2.5"" CEILING THICKNESS",BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,3,4,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92218-BM,E3SL-LHIMUNV E3SLBD92218-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92218-NBM,E3SL-LHIMUNV E3SLBD92218-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92218-WM,E3SL-LHIMUNV E3SLBD92218-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92418-BM,E3SL-LHIMUNV E3SLBD92418-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92418-NBM,E3SL-LHIMUNV E3SLBD92418-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92418-WM,E3SL-LHIMUNV E3SLBD92418-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92718-BM,E3SL-LHIMUNV E3SLBD92718-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92718-NBM,E3SL-LHIMUNV E3SLBD92718-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92718-WM,E3SL-LHIMUNV E3SLBD92718-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93018-BM,E3SL-LHIMUNV E3SLBD93018-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93018-NBM,E3SL-LHIMUNV E3SLBD93018-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93018-WM,E3SL-LHIMUNV E3SLBD93018-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93518-BM,E3SL-LHIMUNV E3SLBD93518-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93518-NBM,E3SL-LHIMUNV E3SLBD93518-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93518-WM,E3SL-LHIMUNV E3SLBD93518-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD9WD18-BM,E3SL-LHIMUNV E3SLBD9WD18-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD9WD18-NBM,E3SL-LHIMUNV E3SLBD9WD18-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD9WD18-WM,E3SL-LHIMUNV E3SLBD9WD18-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92225-BM,E3SL-LHIMUNV E3SLBD92225-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92225-NBM,E3SL-LHIMUNV E3SLBD92225-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92225-WM,E3SL-LHIMUNV E3SLBD92225-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92425-BM,E3SL-LHIMUNV E3SLBD92425-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92425-NBM,E3SL-LHIMUNV E3SLBD92425-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92425-WM,E3SL-LHIMUNV E3SLBD92425-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92725-BM,E3SL-LHIMUNV E3SLBD92725-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92725-NBM,E3SL-LHIMUNV E3SLBD92725-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92725-WM,E3SL-LHIMUNV E3SLBD92725-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93025-BM,E3SL-LHIMUNV E3SLBD93025-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93025-NBM,E3SL-LHIMUNV E3SLBD93025-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93025-WM,E3SL-LHIMUNV E3SLBD93025-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93525-BM,E3SL-LHIMUNV E3SLBD93525-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93525-NBM,E3SL-LHIMUNV E3SLBD93525-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93525-WM,E3SL-LHIMUNV E3SLBD93525-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD9WD25-BM,E3SL-LHIMUNV E3SLBD9WD25-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD9WD25-NBM,E3SL-LHIMUNV E3SLBD9WD25-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD9WD25-WM,E3SL-LHIMUNV E3SLBD9WD25-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92240-BM,E3SL-LHIMUNV E3SLBD92240-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92240-NBM,E3SL-LHIMUNV E3SLBD92240-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92240-WM,E3SL-LHIMUNV E3SLBD92240-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92440-BM,E3SL-LHIMUNV E3SLBD92440-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92440-NBM,E3SL-LHIMUNV E3SLBD92440-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92440-WM,E3SL-LHIMUNV E3SLBD92440-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92740-BM,E3SL-LHIMUNV E3SLBD92740-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92740-NBM,E3SL-LHIMUNV E3SLBD92740-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92740-WM,E3SL-LHIMUNV E3SLBD92740-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93040-BM,E3SL-LHIMUNV E3SLBD93040-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93040-NBM,E3SL-LHIMUNV E3SLBD93040-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93040-WM,E3SL-LHIMUNV E3SLBD93040-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93540-BM,E3SL-LHIMUNV E3SLBD93540-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93540-NBM,E3SL-LHIMUNV E3SLBD93540-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93540-WM,E3SL-LHIMUNV E3SLBD93540-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD9WD40-BM,E3SL-LHIMUNV E3SLBD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD9WD40-NBM,E3SL-LHIMUNV E3SLBD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD9WD40-WM,E3SL-LHIMUNV E3SLBD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LOIMUNV E3SLBD92240-BM,E3SL-LOIMUNV E3SLBD92240-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LOIMUNV E3SLBD92240-NBM,E3SL-LOIMUNV E3SLBD92240-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LOIMUNV E3SLBD92240-WM,E3SL-LOIMUNV E3SLBD92240-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LOIMUNV E3SLBD92440-BM,E3SL-LOIMUNV E3SLBD92440-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LOIMUNV E3SLBD92440-NBM,E3SL-LOIMUNV E3SLBD92440-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LOIMUNV E3SLBD92440-WM,E3SL-LOIMUNV E3SLBD92440-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LOIMUNV E3SLBD92740-BM,E3SL-LOIMUNV E3SLBD92740-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LOIMUNV E3SLBD92740-NBM,E3SL-LOIMUNV E3SLBD92740-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LOIMUNV E3SLBD92740-WM,E3SL-LOIMUNV E3SLBD92740-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LOIMUNV E3SLBD93040-BM,E3SL-LOIMUNV E3SLBD93040-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LOIMUNV E3SLBD93040-NBM,E3SL-LOIMUNV E3SLBD93040-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LOIMUNV E3SLBD93040-WM,E3SL-LOIMUNV E3SLBD93040-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LOIMUNV E3SLBD93540-BM,E3SL-LOIMUNV E3SLBD93540-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LOIMUNV E3SLBD93540-NBM,E3SL-LOIMUNV E3SLBD93540-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LOIMUNV E3SLBD93540-WM,E3SL-LOIMUNV E3SLBD93540-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LOIMUNV E3SLBD9WD40-BM,E3SL-LOIMUNV E3SLBD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LOIMUNV E3SLBD9WD40-NBM,E3SL-LOIMUNV E3SLBD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LOIMUNV E3SLBD9WD40-WM,E3SL-LOIMUNV E3SLBD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92260-BM,E3SL-LHIMUNV E3SLBD92260-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92260-NBM,E3SL-LHIMUNV E3SLBD92260-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92260-WM,E3SL-LHIMUNV E3SLBD92260-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92460-BM,E3SL-LHIMUNV E3SLBD92460-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92460-NBM,E3SL-LHIMUNV E3SLBD92460-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92460-WM,E3SL-LHIMUNV E3SLBD92460-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD92760-BM,E3SL-LHIMUNV E3SLBD92760-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD92760-NBM,E3SL-LHIMUNV E3SLBD92760-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD92760-WM,E3SL-LHIMUNV E3SLBD92760-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93060-BM,E3SL-LHIMUNV E3SLBD93060-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93060-NBM,E3SL-LHIMUNV E3SLBD93060-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93060-WM,E3SL-LHIMUNV E3SLBD93060-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD93560-BM,E3SL-LHIMUNV E3SLBD93560-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD93560-NBM,E3SL-LHIMUNV E3SLBD93560-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD93560-WM,E3SL-LHIMUNV E3SLBD93560-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SL-LHIMUNV E3SLBD9WD60-BM,E3SL-LHIMUNV E3SLBD9WD60-BM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SL-LHIMUNV E3SLBD9WD60-NBM,E3SL-LHIMUNV E3SLBD9WD60-NBM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SL-LHIMUNV E3SLBD9WD60-WM,E3SL-LHIMUNV E3SLBD9WD60-WM,"ELEMENT 3"" SQUARE",FLANGELESS,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92218-BM,E3SWC-LHIMUNV E3SLBD92218-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,BLACK BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92218-NBM,E3SWC-LHIMUNV E3SLBD92218-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,NATURAL BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92218-WM,E3SWC-LHIMUNV E3SLBD92218-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",18°,WHITE BRASS,729,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92418-BM,E3SWC-LHIMUNV E3SLBD92418-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,BLACK BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92418-NBM,E3SWC-LHIMUNV E3SLBD92418-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,NATURAL BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92418-WM,E3SWC-LHIMUNV E3SLBD92418-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",18°,WHITE BRASS,1008,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92718-BM,E3SWC-LHIMUNV E3SLBD92718-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,BLACK BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92718-NBM,E3SWC-LHIMUNV E3SLBD92718-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,NATURAL BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92718-WM,E3SWC-LHIMUNV E3SLBD92718-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",18°,WHITE BRASS,1094,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93018-BM,E3SWC-LHIMUNV E3SLBD93018-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,BLACK BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93018-NBM,E3SWC-LHIMUNV E3SLBD93018-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93018-WM,E3SWC-LHIMUNV E3SLBD93018-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",18°,WHITE BRASS,1215,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93518-BM,E3SWC-LHIMUNV E3SLBD93518-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,BLACK BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93518-NBM,E3SWC-LHIMUNV E3SLBD93518-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,NATURAL BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93518-WM,E3SWC-LHIMUNV E3SLBD93518-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",18°,WHITE BRASS,1337,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD9WD18-BM,E3SWC-LHIMUNV E3SLBD9WD18-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,BLACK BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD9WD18-NBM,E3SWC-LHIMUNV E3SLBD9WD18-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,NATURAL BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD9WD18-WM,E3SWC-LHIMUNV E3SLBD9WD18-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",18°,WHITE BRASS,1215,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD18-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92225-BM,E3SWC-LHIMUNV E3SLBD92225-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,BLACK BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92225-NBM,E3SWC-LHIMUNV E3SLBD92225-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,NATURAL BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92225-WM,E3SWC-LHIMUNV E3SLBD92225-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",25°,WHITE BRASS,810,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92425-BM,E3SWC-LHIMUNV E3SLBD92425-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,BLACK BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92425-NBM,E3SWC-LHIMUNV E3SLBD92425-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,NATURAL BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92425-WM,E3SWC-LHIMUNV E3SLBD92425-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",25°,WHITE BRASS,1121,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92725-BM,E3SWC-LHIMUNV E3SLBD92725-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,BLACK BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92725-NBM,E3SWC-LHIMUNV E3SLBD92725-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,NATURAL BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92725-WM,E3SWC-LHIMUNV E3SLBD92725-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",25°,WHITE BRASS,1215,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93025-BM,E3SWC-LHIMUNV E3SLBD93025-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,BLACK BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93025-NBM,E3SWC-LHIMUNV E3SLBD93025-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93025-WM,E3SWC-LHIMUNV E3SLBD93025-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",25°,WHITE BRASS,1350,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93525-BM,E3SWC-LHIMUNV E3SLBD93525-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,BLACK BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93525-NBM,E3SWC-LHIMUNV E3SLBD93525-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,NATURAL BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93525-WM,E3SWC-LHIMUNV E3SLBD93525-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",25°,WHITE BRASS,1485,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD9WD25-BM,E3SWC-LHIMUNV E3SLBD9WD25-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,BLACK BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD9WD25-NBM,E3SWC-LHIMUNV E3SLBD9WD25-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,NATURAL BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD9WD25-WM,E3SWC-LHIMUNV E3SLBD9WD25-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",25°,WHITE BRASS,1350,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD25-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92240-BM,E3SWC-LHIMUNV E3SLBD92240-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92240-NBM,E3SWC-LHIMUNV E3SLBD92240-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92240-WM,E3SWC-LHIMUNV E3SLBD92240-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,855,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92440-BM,E3SWC-LHIMUNV E3SLBD92440-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92440-NBM,E3SWC-LHIMUNV E3SLBD92440-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92440-WM,E3SWC-LHIMUNV E3SLBD92440-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,1183,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92740-BM,E3SWC-LHIMUNV E3SLBD92740-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92740-NBM,E3SWC-LHIMUNV E3SLBD92740-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92740-WM,E3SWC-LHIMUNV E3SLBD92740-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,1283,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93040-BM,E3SWC-LHIMUNV E3SLBD93040-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93040-NBM,E3SWC-LHIMUNV E3SLBD93040-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93040-WM,E3SWC-LHIMUNV E3SLBD93040-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1425,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93540-BM,E3SWC-LHIMUNV E3SLBD93540-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93540-NBM,E3SWC-LHIMUNV E3SLBD93540-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93540-WM,E3SWC-LHIMUNV E3SLBD93540-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1568,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD9WD40-BM,E3SWC-LHIMUNV E3SLBD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD9WD40-NBM,E3SWC-LHIMUNV E3SLBD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD9WD40-WM,E3SWC-LHIMUNV E3SLBD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1425,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LOIMUNV E3SLBD92240-BM,E3SWC-LOIMUNV E3SLBD92240-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,BLACK BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LOIMUNV E3SLBD92240-NBM,E3SWC-LOIMUNV E3SLBD92240-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,NATURAL BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LOIMUNV E3SLBD92240-WM,E3SWC-LOIMUNV E3SLBD92240-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",40°,WHITE BRASS,651,2200K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LOIMUNV E3SLBD92440-BM,E3SWC-LOIMUNV E3SLBD92440-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,BLACK BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LOIMUNV E3SLBD92440-NBM,E3SWC-LOIMUNV E3SLBD92440-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,NATURAL BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LOIMUNV E3SLBD92440-WM,E3SWC-LOIMUNV E3SLBD92440-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",40°,WHITE BRASS,901,2400K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LOIMUNV E3SLBD92740-BM,E3SWC-LOIMUNV E3SLBD92740-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,BLACK BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LOIMUNV E3SLBD92740-NBM,E3SWC-LOIMUNV E3SLBD92740-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,NATURAL BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LOIMUNV E3SLBD92740-WM,E3SWC-LOIMUNV E3SLBD92740-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",40°,WHITE BRASS,977,2700K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LOIMUNV E3SLBD93040-BM,E3SWC-LOIMUNV E3SLBD93040-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,BLACK BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LOIMUNV E3SLBD93040-NBM,E3SWC-LOIMUNV E3SLBD93040-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,NATURAL BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LOIMUNV E3SLBD93040-WM,E3SWC-LOIMUNV E3SLBD93040-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",40°,WHITE BRASS,1085,3000K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LOIMUNV E3SLBD93540-BM,E3SWC-LOIMUNV E3SLBD93540-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,BLACK BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LOIMUNV E3SLBD93540-NBM,E3SWC-LOIMUNV E3SLBD93540-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,NATURAL BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LOIMUNV E3SLBD93540-WM,E3SWC-LOIMUNV E3SLBD93540-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",40°,WHITE BRASS,1194,3500K,12W,12,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LOIMUNV E3SLBD9WD40-BM,E3SWC-LOIMUNV E3SLBD9WD40-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,BLACK BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LOIMUNV E3SLBD9WD40-NBM,E3SWC-LOIMUNV E3SLBD9WD40-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,NATURAL BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LOIMUNV E3SLBD9WD40-WM,E3SWC-LOIMUNV E3SLBD9WD40-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"LOW OUTPUT, 12W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",40°,WHITE BRASS,1085,3000K,12W,12,E3SF-LOIMUNV E3SFBD9WD40-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92260-BM,E3SWC-LHIMUNV E3SLBD92260-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,BLACK BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92260-NBM,E3SWC-LHIMUNV E3SLBD92260-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,NATURAL BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92260-WM,E3SWC-LHIMUNV E3SLBD92260-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2200K, 2-STEP",60°,WHITE BRASS,741,2200K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92460-BM,E3SWC-LHIMUNV E3SLBD92460-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,BLACK BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92460-NBM,E3SWC-LHIMUNV E3SLBD92460-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,NATURAL BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92460-WM,E3SWC-LHIMUNV E3SLBD92460-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2400K, 2-STEP",60°,WHITE BRASS,1025,2400K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD92760-BM,E3SWC-LHIMUNV E3SLBD92760-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,BLACK BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD92760-NBM,E3SWC-LHIMUNV E3SLBD92760-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,NATURAL BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD92760-WM,E3SWC-LHIMUNV E3SLBD92760-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 2700K, 1-STEP",60°,WHITE BRASS,1112,2700K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93060-BM,E3SWC-LHIMUNV E3SLBD93060-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,BLACK BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93060-NBM,E3SWC-LHIMUNV E3SLBD93060-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93060-WM,E3SWC-LHIMUNV E3SLBD93060-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K, 1-STEP",60°,WHITE BRASS,1235,3000K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD93560-BM,E3SWC-LHIMUNV E3SLBD93560-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,BLACK BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD93560-NBM,E3SWC-LHIMUNV E3SLBD93560-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,NATURAL BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD93560-WM,E3SWC-LHIMUNV E3SLBD93560-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3500K, 1-STEP",60°,WHITE BRASS,1359,3500K,16.2W,16.2,Contact Manufacturer for IES File,4,1,Metal - Visual Comfort & Co. - White Brass
E3SWC-LHIMUNV E3SLBD9WD60-BM,E3SWC-LHIMUNV E3SLBD9WD60-BM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,BLACK BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,4,1,Metal - Visual Comfort & Co. - Black Brass
E3SWC-LHIMUNV E3SLBD9WD60-NBM,E3SWC-LHIMUNV E3SLBD9WD60-NBM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,NATURAL BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,4,1,Metal - Visual Comfort & Co. - Natural Brass
E3SWC-LHIMUNV E3SLBD9WD60-WM,E3SWC-LHIMUNV E3SLBD9WD60-WM,"ELEMENT 3"" SQUARE",FLANGELESS WOOD CEILING,"HIGH OUTPUT, 16W",UNIVERSAL PHASE/0-10V 1%,"ELEMENT 3"" SQUARE MARINE",FLANGELESS,BEVEL,FIXED DOWNLIGHT,"90 CRI, 3000K-1800K, WARM DIM, 2-STEP1",60°,WHITE BRASS,1235,3000K,16.2W,16.2,E3SF-LHIMUNV E3SFBD9WD60-WM.ies,4,1,Metal - Visual Comfort & Co. - White Brass
